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Dated: ___________________________



Technical Proposal
People’s Primary Healthcare Initiative (PPHI) - Balochistan



ESTABLISHMENT OF DISTRICT OFFICES AND MAJOR AND MINOR CIVIL WORKS OF BASIC HEALTH UNITS (BHUs), AND DISTRICT WAREHOUSE UNDER PPHI-BALOCHISTAN, 2026.


       NAME OF BIDDER: _______________________________________
              (To be filled-in by the Bidder)








   Address: People’s Primary Healthcare Initiative (PPHI) - Balochistan 
                          House # 8-A, Jinnah Town, Samungli Road, Quetta-Pakistan.

Phone:	081-2863620
Website: 	www.pphib.org


LETTER OF INVITATION FOR BIDS:
Sealed proposals are invited from eligible bidders for major and minor civil works at (21) Twenty BHUs, (01) one DO, and (02) one district warehouse PPHI-Balochistan, under the People’s Primary Healthcare Initiative (PPHI)-Balochistan in accordance with the applicable procurement rules and policies of PPHI-Balochistan. Firms having proven experience in the execution of major and minor civil works and construction also duly registered with the Pakistan Engineering Council (PEC) under the relevant categories and codes are eligible to participate in the bidding process.

	REQUIRED BIDDING INFORMATION
	TO BE FILLED BY THE PEOPLES PRIMARY HEALTHCARE INITIATIVE (PPHI-B)

	DESIGNATION OF PROCUREMENT OFFICER
	DIRECTOR  ADMIN & PROCUREMENT

	POSTAL ADDRESS OF THE PEOPLE’S PRIMARY HEALTH CARE INITIATIVE (PPHI-BALOCHISTAN)
	HOUSE # 8-A, JINNAH TOWN SAMUNGLI ROAD, QUETTA-PAKISTAN.

	PHONE NUMBER & FAX NUMBER
	081-2863620 & 081-2863623

	E-MAIL ADDRESS &WEBSITE
	E-mail: PPHIBLN@GMAIL.COM
Website: https://www.pphib.org

	METHOD OF PROCUREMENT
	SINGLE STAGE - TWO ENVELOPE BIDDING PROCEDURE

	ISSUANCE OF BIDDING DOCUMENTS
	The tender documents can be downloaded from the PPHI-Balochistan website:  http://pphib.org/

	DEADLINE FOR SUBMISSION OF BIDS
	Date: 27th October 2026 & Till 11:00 A.M directly submitted to the Head Office, PPHI-Balochistan.

	OPENING OF TECHNICAL BIDS
	Date: 27th October 2026 & Time 12:00 P.M at the Head Office of PPHI-Balochistan.

	OPENING OF FINANCIAL BIDS
	Date: Shall be communicated to qualified bidders after technical evaluation.

	BIDDING DOCUMENT FEE
	AMOUNT: PKR. 2,000/- PAY ORDER IN THE NAME OF PPHI- Balochistan WITH TECHNICAL BID IN A SEPARATE ENVELOPE. SUBMISSION OF BIDDING DOCUMENT FEE IS MANDATORY WITH TECHNICAL PROPOSAL, 

	BID SECURITY/EARNEST MONEY
	AMOUNT: 2% OF THE QUOTED AMOUNT MANNER OF CALL DEPOSIT/ PAY ORDER IN FAVOR OF PPHI-BALOCHISTAN, MUST BE PART OF FINANCIAL PROPOSAL.



             ELIGIBILITY CRITERIA FOR BIDDERS:
	SR. NO
	BIDDERS ELIGIBILITY FACTOR
	MANDATORY REQUIREMENT
	DOCUMENT REQUIRED

	01
	Legal Status & Tax Registration.
	The bidder must possess a valid NTN Certificate, be registered with the Federal Board of Revenue (FBR) under the relevant tariff/registration category for Construction / Civil Works / Government Contractors, and must be an Active Taxpayer at the time of submission of bid documents.
	Copies of valid NTN Certificate, GST & BSTS Registration Certificate (Where applicable), and Active Taxpayer Profile, duly verifiable from FBR IRIS / official FBR and BRA website.

	02
	Relevant Experience
	Minimum 03 (Three) successfully completed similar Civil Work assignments, having cumulative value not less than PKR. 05 million, during the last Three (03) Years. (FY 2023, 2024, and 2025.)
	Copies of Work Orders and Completion Certificates, clearly mentioning scope, value, and dates, duly attested by Senior Executive of the firm. PPHI-B reserve the right of verification of work orders, completion certificates. 

	03
	Financial Capacity (For Firms)
	Minimum average annual turnover of PKR 10 million during the last three (03) financial years (FY 2023, 2024, and 2025), supported by audited financial statements or Annual tax returns.
	Audited Financial Statements OR Annual Income Tax Return only.

	04
	Non-Blacklisting and disclosure of litigation cases
	Must not be presently black-listed by any Government/ Semi Govt or Private Organization must declare the litigation cases.
	Declaration of Non-blacklisting and disclosure of litigation cases on Non-Judicial Stamp paper by the Bidder/Individual. 

	


05
	PEC Registration 
	The bidder must be registered with the Pakistan Engineering Council (PEC) in an appropriate category and specialization relevant to the scope of civil works (e.g., C-6, C-5 or above). Registration must be valid at the time of bid submission.
	Copy of valid PEC Registration Certificate clearly showing category, specialization, and validity.

	06
	Technical Capacity
	Technical HR (Engineers) with previous experience of similar assignments  as  required  by  the Peoples Primary Health Care Initiative (PPHI-B) in the Data-sheet
	Detailed CVs of the HR/Individual along with PEC registration.
01 Civil Engineer(PEC Registered)
01 Site Supervisor. 

	07
	Work completion compliance
	Must agree to serve the Contract within agreed time i.e., 90 days.
	Completion time must be clearly specified in the Technical Bid.

	
08
	Agreement with all the terms & conditions
	Must unconditionally agree with all the instructions, terms & conditions specified in the bidding documents &
contract agreement
	Signature & company seal on every page of the bidding document.

	09
	Submission of Bidding Document Fee & Bid Security
	As required by the People’s Primary Healthcare Initiative (PPHI-Balochistan) in the Tender Notice.
	AMOUNT: PKR. 2,000/- Tender Fee in separate envelope with technical proposal.
AMOUNT: 2 % Security deposit with financial proposal Only.






NOTE: 
a) It is mandatory for the bidders to score “YES” in all the above-mentioned nine (09) requirements of eligibility. In-case of single “NO” to any requirement, the Bid shall be declared NON-RESPONSIVE resulting disqualification for sample submission and financial bid opening.
b) No document shall be added in bidding documents once bid documents are submitted.
c) Submission of Multiple Bids under a Single Firm (Lot-wise):
i. A Single Bidders may be awarded multiple lots, subject to fulfillment of technical and financial qualification criteria.
ii. Each bid shall complete in all respects and shall be submitted separately, including independent Technical and Financial Proposals along with a separate Call Deposit Receipt (CDR)/Bid Security for each lot. Partial bidding within a lot or submission of incomplete bids shall render the bid non-responsive.
d) Please avoid to attach documents not required in the above mentioned criteria and it would be convenient to tag each eligibility criteria documents.
e) Bidders from other cities/provinces may send their bids via courier at below mentioned mailing address and can participate in the bidding process virtually through online link (subject to prior intimation to the procuring officer) if desired, otherwise physical presence is preferred. 
f) Technical proposals shall not contain any financial proposal information; otherwise the bid shall be rejected.
g) The Procuring Agency reserves the right to reject any or all bids or cancel the procurement proceedings at any time prior to award of contract without disclosing any reason. 
Postal Address: PPHI-B Head Office House # 8-A, Jinnah Town, Samungli Road, Quetta. 



























Bidding Instructions and General Conditions
1. Bid Submission Requirements
a) The bidder must quote for the entire scope of works or lot wise specified in the tender document. Partial, conditional, or incomplete bids shall be rejected.
b) All bids must be tape-bound, properly sealed, and clearly labeled. Each page must be numbered, signed, and stamped by the authorized representative of the firm.
c) All documents shall be attached in the sequence prescribed in the tender document for evaluation purposes.
d) Any interlineations, erasers, or overwriting shall be valid only if initialized by the person(s) signing the bid.
e) Blank fields in the bid forms must be duly filled. Incomplete or unsigned bids shall be treated as non-responsive.
2. Method and Deadline of Submission
a) Preferably, bids shall be submitted by hand through the firm’s authorized representative on or before the date and time specified in the Letter of Invitation. 
b) The bid shall comprise a single package containing two separate envelopes:
a. Technical Proposal
b. Financial Proposal
c) Each envelope shall be sealed and marked in bold letters as “TECHNICAL PROPOSAL” and “FINANCIAL PROPOSAL” (in case of bidding for more than one lot)
d) Both envelopes shall then be placed in an outer sealed envelope clearly marked with the Tender Reference Number and Subject.
e) Bids received after the specified deadline shall be rejected without opening.
3. Conditions for Opening and Validity
a) If the submission or opening date falls on a public holiday or non-working day, the bids shall be opened on the next working day at the same time and venue.
b) A bidder may withdraw its bid before the submission deadline.
I. No withdrawal is permitted after the submission deadline until the expiry of the bid validity period.
II. Any withdrawal during the validity period at any stage may lead to legal action under applicable rules of   PPHI-B.
4. Eligibility of Bidders
a) The invitation is open to all firms registered with the Federal Board of Revenue (FBR) under the relevant registration/tariff category for Construction / Civil Works / Government Contractors, subject to fulfillment of all mandatory eligibility criteria.
b) Bidders must have demonstrated experience in the execution and completion of major and/or minor civil works for government, semi-government, institutional, or similar organizations.
c) Bidders under declaration of ineligibility, suspension, or blacklisting by any government, regulatory authority, or other organization are not eligible to participate.



5. Blacklisting and Debarment
The following actions shall render a bidder liable for blacklisting/debarment:
a) Submission of false, fabricated, or forged documents or misrepresentation of facts at any stage of the bidding or contract execution.
b) Failure to execute the civil works in accordance with the approved drawings, technical specifications, quality standards, BOQs, or agreed completion schedule.
c) Persistent non-compliance with contract terms or specifications.
d) Engagement in corrupt, fraudulent, or unethical practices.
e) Bid rigging, tender fixing, or any conduct detrimental to the integrity and transparency of the procurement process.
f) Any security-related concerns or actions that adversely affect the reputation of the Procuring Agency or the State.
6. Clarifications and Amendments
a) A prospective bidder may seek clarification(s) in writing not later than seven (7) days prior to the submission deadline at the Procuring Agency’s address indicated in the Bid Data Sheet.
b) The Procuring Agency shall issue written responses (without disclosing the identity of the inquirer) to all bidders who have obtained the documents no verbal response shell be accepted.
c) The Procuring Agency may, at any time before the submission deadline, amend the bidding documents through a written addendum.
d) Such amendments shall be notified through official correspondence  or publication at the official PPHI-B website.
e) To accommodate the amendment(s), the Procuring Agency may extend the bid submission deadline, if deemed necessary.
7. Corrupt or Fraudulent Practices and Mechanism for Debarment / Blacklisting
A. Definition of Corrupt and Fraudulent Practices
For the purpose of this tender, the following practices shall constitute corrupt, fraudulent, coercive, collusive, or obstructive behavior, which are strictly prohibited:
a) Corrupt Practice: Offering, giving, receiving, or soliciting directly or indirectly anything of value to influence the actions of a public official, procuring entity, or any party in the procurement process or contract execution for wrongful gain.
b) Fraudulent Practice: Any act, omission, or misrepresentation that knowingly or recklessly misleads or attempts to mislead another party to obtain undue advantage or avoid an obligation.
c) Collusive Practice: Any agreement or arrangement between two or more parties designed to establish bid prices at non-competitive, artificial levels to the detriment of fair competition.
d) Coercive Practice: Direct or indirect actions, threats, or harm to any party or its property to improperly influence their participation or decisions in the procurement process.
e) Obstructive Practice: Deliberate acts intended to impede investigation or audit processes, including falsifying or concealing evidence, making false statements, or intimidating witnesses.
8. Bid Price
a) Price Indication: The bidder shall indicate, in the prescribed form, the unit rates (where applicable), BOQ rates, and the total bid price.
b) Completion and Authentication: The Bill of Quantities (BOQ) and price schedules must be carefully filled, preferably typed, and signed and stamped on each page by the authorized representative of the bidder.
c) Compliance with Technical Specifications: Bids must comply with all approved drawings, technical specifications, and BOQ requirements. Any deviation shall render the bid non-responsive.
d) Inclusive Pricing: Prices must be quoted on a complete execution basis and shall include all applicable taxes, duties, levies, transportation, site establishment, tools and incidental costs necessary for execution of the works at the designated BHUs of PPHI-Balochistan.
e) Tax Exemptions: Any exemption or reduction in taxes or duties available under law shall be passed on to the Procuring Agency.
f) Total Service Requirement: Prices must be quoted for the entire scope of civil works of each lot as defined in the tender documents. Partial, conditional, or incomplete offers shall be considered non-responsive and rejected.
9. Bid Security
The bidder shall submit a bid security amount equal to 2% of the total quoted bid price for each lot, in favor of PPHI-Balochistan. The bid security shall be submitted as part of the Financial Bid only.
10. Bid Validity
a. Bids shall remain valid for 90 days from the date of opening of bid.
b. Bidders agreeing to extend validity must not change the substance of their bids.
c. Bidders declining to extend may withdraw without forfeiting bid security.
      Bidders who:-
a) Agree to the Procuring Agency’s request for extension of bid validity period shall not be permitted to change the substance of their bids; and 
b) Do not agree to an extension of the bid validity period shall be allowed to withdraw their bids without forfeiture of their bid securities. 
11.  Sub-Contracting, Subletting Clause  
The bidder shall not assign, transfer, or sublet the whole or any part of the contract without the prior written approval of the Procuring Agency to subcontractor. 
Any subletting or subcontracting carried out without such approval shall constitute a material violation of the Contract and shall render the Contractor liable to termination of the Contract, forfeiture of Performance Security, blacklisting, and any other action permissible under the prevailing procurement rules and laws.







BIDDER’S INFORMATION: (To be filled-in by the Bidder)

1. Name of company/Individual: __________						______

2. Complete Postal Address:							______	___									______	_____	___									__________________________________________

3. Tel No:				____	4. Email address:			______	______

5.    Fax No: ____					6. Mobile No: 	_______________________	

7. 	Authorized Representative’s name & designation: 


8. 	Type of Business: 
	 (1)    Sole Proprietorship           □ 	(2)         Partnership 	     □
	 (3)    Corporation (Private Ltd.) □	(4)         Corporation (Public Ltd.) □

9. National Tax Number& Date of issuance: _		_____________________________

10. Sales Tax Registration No. GST.________________________________________________

11. Sales Tax Registration No. BRA._______________________________________________

12. Bid Validity   _______________________________ (Please specify in no. of days)

13. Total Completion Time______________________________ (Date of completion)


DELIVERY SCHEDULE CONDITIONS

1. Scope of Delivery & Locations
The successful bidder shall be responsible for the execution and completion of all civil works in accordance with the approved technical specifications, and Bill of Quantities (BOQ) at the designated sites of PPHI-Balochistan as specified in the Tender Document.
2. Completion Time & Work Schedule
A) Contract Period
a. The successful bidder shall complete execution of all civil works at the designated sites of PPHI-Balochistan within 90 (ninety) days from the date of issuance of the Work Order.
b. Works shall be carried out strictly in accordance with the approved work schedule and construction program, unless an extension is granted in writing by PPHI-Balochistan.
B) Phased Based Execution
a. Phased or milestone-based execution may be permitted only with prior written approval of PPHI-Balochistan.
b. Each approved phase/milestone shall remain within the overall contract period of 90 days.
C) Execution & Progress Documentation
The bidder shall submit:
· Work Completion Certificates
· Final Completion Report duly signed by the Engineer / Authorized Representative of PPHI-Balochistan

D) Penalty for Delay
Delay beyond the stipulated 90-day period, excluding delays approved in writing or arising from force majeure, shall attract liquidated damages at the rate of 0.25% per day of the value of the uncompleted portion of works, subject to a maximum of 10% of the total contract value.
E) Force Majeure
Delays caused by events beyond the bidder’s control, including natural disasters, civil disturbances, acts of government, strikes, or other force majeure circumstances, must be immediately reported in writing to PPHI-Balochistan with supporting evidence. A reasonable extension may be granted at the discretion of PPHI-Balochistan.

F) Defects, Damages & Loss
The bidder shall be fully responsible for any damage, defects, poor workmanship, or loss occurring during execution of the works. Any defective or non-compliant work shall be rectified or replaced at the bidder’s cost, or the equivalent cost shall be deducted from the payable amount, as determined by PPHI-Balochistan. PPHI-Balochistan will consider the delivery of contract once 100% work completion report signed by the representative of PPHI-Balochistan and Vendor. In Case of any damaged/Loss/Theft/destruction before 100% work completion and signing of work completion certificate will not be responsibility of PPHI-Balochistan.
3. Place & Mode of Execution
The successful bidder shall be solely responsible for the mobilization of all materials, equipment, and manpower to the designated work sites as specified in the tender documents. The bidder shall ensure safe execution, completion, and handover of the works in strict accordance with the approved technical specifications, and applicable standards.
The bidder shall also provide all required tools, plant, safety gear, and qualified technical staff necessary for proper execution of the works. All arrangements relating to site establishment, storage, handling of materials, safety, and execution logistics shall be the sole responsibility of the bidder.
4. Equipment & Site Handling Requirements
The Bidder must ensure:
a. Availability of appropriate construction equipment, machinery, and tools required for timely and quality execution of the works.
b. Proper storage, protection, and handling of construction materials to prevent damage, deterioration, or misuse.
5. Monitoring & Reporting
The Bidder shall:
a. Provide regular progress updates and reports as required by PPHI-Balochistan.
b. Immediately report any delay, accident, defect, or incident affecting the execution of works.
c. Submit Final Completion Confirmation duly acknowledged by the Engineer / Authorized Representative of PPHI-Balochistan.







DATA-SHEET OF THE ASSIGNMENT / SCOPE OF WORK
The objective of this Data Sheet / Schedule of Requirements is to provide bidders with comprehensive and clear information to fully understand the complete scope of this Work. It ensures that all requirements of the People’s Primary Healthcare Initiative (PPHI-Balochistan) related to the execution, materials, workmanship, timelines, and delivery of works are clearly defined, specified, and duly incorporated, leaving no requirement unaddressed.
It is mandatory for the bidders to meet the following given specifications. All offers meeting or exceeding the following minimum required specification shall be considered for further evaluations in accordance with the evaluation criteria.
The civil works under this tender shall be executed on a Lot-wise basis, as detailed in the Data Sheet and attached BOQs. Bidders may quote for multiple; however, separate financial bids for each Lot shall be submitted. PPHI-Balochistan reserves the right to award the contract for one or multiple Lots to a single bidder, subject to availability of funds and satisfactory evaluation.
District-wise List of Sites – PPHI-Balochistan
	Lot. No
	District Name
	Sr. No.
	Name of Site
	BOQs Attached 

	1
	Kech
	1
	BHU KUNCHATTI
	Attached at Pg.no 21-23

	2
	Dera Bugti
	1
	BHU SHAMOLE
	Attached at Pg.no 24-28

	
	
	2
	BHU HABIB RAHI
	Attached at Pg.no 29-33

	
	
	3
	BHU JANI KHAN
	Attached at Pg.no 34-41

	
	
	4
	BHU MARROW
	Attached at Pg.no 42-45

	
	
	5
	BHU PEER KOH
	Attached at Pg.no 46-50

	
	
	6
	BHU PEETOKH
	Attached at Pg.no 51-53

	
	
	7
	BHU SERLOPE
	Attached at Pg.no 54-56

	
	
	8
	DO DERA BUGTI (ADDITIONAL WORK)
	Attached at Pg.no 57-63

	
	
	9
	WAREHOUSE
	Attached at Pg.no 64-66

	3
	Gawadar
	1
	BHU ZAHRAN
	Attached at Pg.no 67-71

	4
	Upper Dera Bughti
	1
	DISTRICT OFFICE
	Attached at Pg.no 72-78

	5
	Barshor
	2
	DISTRICT OFFICE
	Attached at Pg.no 79-83



INSTRUCTIONS FOR PREPARING TECHNICAL BID
These Instructions are being given for strict compliance by the Bidders. Failure to fulfill any instruction given here-under may result in dis-qualification of the Bid/s. 
Proposals shall be prepared on following lines: -	
1. Sealed Envelope containing the Technical Proposal should clearly state:
a. “Name of Bidder _________”
b. “Name of Tender_________” 
c. “TECHNICAL PROPOSAL”
2. The portion of Technical Proposal of this bidding document duly filled, supported with Bidder’s covering Letter and the technical Bid on Bidders Letter Head be attached as the Technical Proposal.
3. Technical Proposal shall be prepared keeping in view the specifications provided in the Data Sheet and the schedule of requirements or otherwise as placed demand further during the bidding process.
4. Following information should be attached/contained in the Technical Proposal: -
a. Receipt of payment of bidding Document Fee May be in terms of Pay Order in favor of PPHI BALOCHISTAN.
b. Completion time/Delivery time, which means; actual execution time for the titled Work. 
c. Documentary evidence of fulfillment of eligibility criteria for Bidders as required by the Peoples Primary Healthcare Initiative, Balochistan. (PPHI-Balochistan).
d. Documentary evidence of fulfillment of complete schedule of requirements as per evaluation criteria including technical, administrative and service requirements of the Peoples Primary Healthcare Initiative, Balochistan (PPHI-Balochistan)
e. Description of status as Partnership / authorization from the Firm / authorized importer / distributor / manufacturer / retailer etc. (as the case may be) as required by the People’s Primary Healthcare Initiative, Balochistan (PPHI-Balochistan) in the schedule of requirements.
f. Defect Liability Period: details. (As applicable) as required by the Peoples Primary Healthcare Initiative, Balochistan (PPHI-Balochistan) in the schedule of requirements as mentioned. 
g. Every page of the Bid must be numbered, signed & stamped by the authorized representative.
5. Attachment of any document not demanded by the Peoples Primary Healthcare Initiative (PPHI-Balochistan) at instruction  of “Instruction for preparation of Technical Bid” is strictly prohibited.

Evaluation Criteria: Selection of the successful bidder shall be based on the Single Stage-Two Envelop Method 

The procedure shall be applied as follows: -
1. Bidders Eligibility Assessment. Initial evaluation of the technical proposals shall be carried-out by the PROCUREMENT COMMITTEE, as per the requirements of the eligibility criteria laid down under the heading of “Letter of Invitation for Bids – Eligibility Criteria for Bidders” in the following manner:
	Sr. No.
	Bidders Eligibility Factor
	Requirement 
	Documents Attached

	
	
	
	YES
	NO

	01
	Legal Status & Tax Registration.
	Copies of valid NTN Certificate, GST & BSTS Registration Certificate (Where applicable), and Active Taxpayer Profile, duly verifiable from FBR IRIS / official FBR and BRA website.
	
	

	02
	Relevant Experience
	Copies of Work Orders and Completion Certificates, clearly mentioning scope, value, and dates, duly attested by Senior Executive of the firm. 
	
	

	03
	Financial Capacity (For Firms)
	Audited Financial Statements OR Annual Income Tax Return only showing the bidder have an average turnover of PKR 15 Million for the last 03 years (2023,2024,2025)
	
	

	           04
	Non-Blacklisting and disclosure of litigation cases
	Declaration of Non-blacklisting and disclosure of litigation cases on Non Judicial Stamp paper by the Bidder/Individual.
	
	

	05
	PEC Registration 
	Copy of valid PEC Registration Certificate clearly showing category, specialization, and validity.
	
	

	06
	Technical Capacity
	Detailed CVs of the HR/Individual along with PEC registration. 01 Civil Engineer(PEC Registered) 01 Site Supervisor.
	
	

	07
	Delivery time compliance
	Completion time must be clearly specified in the Technical Bid. i-e 90 Days.
	
	

	08
	Agreement with all the terms & conditions
	Signature & company seal on every page of the bidding document.
	
	

	09
	Submission of Bidding Document Fee & Bid Security
	As required by the People’s Primary Healthcare Initiative (PPHI-Balochistan) in the Tender Notice.
	
	


i. Firm must score “YES” in all requirements of the eligibility criteria to be categorized as Eligible. “NO” to any requirement of the eligibility criteria, by any bidder shall render the Firm as Ineligible.
ii. Subsequent upon said assessment, Bidders shall be categorized as:
1. Eligible Bidders
2. Ineligible Bidders
2. Return of Non-Responsive Proposals & preparation of Technical Evaluation Report. Technical Proposals not conforming to the required technical, administrative or legal requirements shall be declared as “Disqualified” and consequently shall NOT be accepted for any further evaluation:
i. Their financial proposals shall be returned without being opened. 
ii. Their Bid security shall be released upon their written request.
iii. Technical Evaluation Report, shall be prepared duly signed by all the members of the Procurement Committee, giving REASONS for;
1. Acceptance of the Eligible Bid/s and.
2. Rejection of the Ineligible Bid/s.
iv. Technical Evaluation concludes at this stage.

3. Recommendation of Procurement Committee 

	After Technical Qualification, the contract will be awarded to the “Lowest Financially Evaluated bidder” with minimum quoted rates among all the Technical qualified Contractors. 

Note
BID GRIEVENCES
				Any bidder having any grievance over the tender/evaluation process, may present the same in black and white to the “Grievance Redressal Committee” through the Chief Executive Officer PPHI-Balochistan at any stage.  







[image: ]          The Head Office,
          People’s Primary Healthcare Initiative, Balochistan.
          Admin Section
          Ref No. PPHI-B/H.O-BLN/CW/2025-26/04
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Financial Proposal 
People’s Primary Healthcare Initiative (PPHI) - Balochistan



ESTABLISHMENT OF DISTRICT OFFICES AND MAJOR AND MINOR CIVIL WORKS OF BASIC HEALTH UNITS (BHUs), AND DISTRICT WAREHOUSE UNDER PPHI-BALOCHISTAN, 2026.





      NAME OF BIDDER: _______________________________________
         (To be filled-in by the Bidder)






              Address: Peoples Primary Healthcare Initiative (PPHI) Balochistan  
                            House # 8-A, Jinnah Town Samungli Road, Quetta-Pakistan.

                                                         Phone: 081-2863620
Website: www.pphib.org

1. Name of company: __________						___________

2. Complete Postal Address: 							______	___									______	_____	___					____________	_____________________________________________________

3. Tel No:				____	4. Email address:			________	

5.    Fax No: ____					6. Mobile No: 	______________________

2. Authorized Representative’s name & designation: 
__________________________________________

8. 	Type of Business: 
	 (1)    Sole Proprietorship           □ 	(2)         Partnership 	     □
	 (3)    Corporation (Private Ltd.) □	(4)         Corporation (Public Ltd) □

9. National Tax Number& Date of issuance: _			_____________________________

10. Sales Tax Registration No. / BRA Registration No.____________________________

11. GST No. ________________________________________________

12. BRA No. ________________________________________________

13. Bid Validity: __________ (Please specify in No. of Days)

14. Total Bid Value: _________________ (In Pakistani Rupees)

INSTRUCTIONS FOR PREPARING FINANCIAL PROPOSAL
	These Instructions are being given for strict compliance by the Bidders. Failure to fulfill any instruction given here-under may result in disqualification of the Bid/s. 
Financial Proposals shall be prepared on following lines: - 	
1. Sealed Envelope containing the Financial Proposal should clearly state:
a. “Name of Bidder _________”
b. “Name of Tender_________” 
c. “Financial Proposal”
2. The portion of Financial Proposal of this bidding document duly filled, supported with Bidder’s covering Letter be attached as the Financial Proposal of the bidder.
3. Following information should be attached/contained in the financial proposal: -
a. Original Bid Security (If required by the Peoples Primary Health Initiative (PPHI-Balochistan).
b. Taxes must be included along-with the price of each item.
c. Financial Bid shall be prepared on the Bidders Letter Head in the BOQs format attached in tender and needs to be provide in the financial proposal.
[bookmark: _Hlk143778838]Note: Each Bidder must mention clearly the applicable rate of BRA & GST on each item of its Bid.
4. Offer must be quoted on TCA (Total Cost of Acquisition) basis at the risk & cost of the bidder. This means:
i. ALL costs (including duties, taxes & other Govt. payables) incurred up-to delivery at the designated location of the Peoples Primary Health Initiative (PPHI-B).
ii. Complete services as required in the schedule of requirements of this bidding document. 
iii. Cost including fixation, assembling, dismantling etc. (As & where applicable).
5. BST/GST Taxes must be included along-with the price of each item/components/service.
6. In-case of any Tax exemptions, exemption certificate from the concerned Tax Office / Regional Tax Office pertaining particularly to this case may be provided; otherwise, taxes shall be deducted as per Government Policy / Rules.
7. Financial Evaluation. Financial Proposals of the Responsive Technical Proposals shall be publicly opened of Technically qualified bidders in the next meeting as specified in this document under the heading of “Letter of Invitation for Bid” Financial Comparative Statement / Evaluation Report of the “Responsive Proposals” shall be prepared by the PROCUREMENT COMMITTEE in the following manner:
Financial Evaluation Criteria
	Lot No. 01

	Sr. No
	BOQ Reference
	Qualified Bidder 1 (Total Price – PKR) incl. all taxes
	Qualified Bidder 2 (Total Price – PKR)
Incl. all taxes
	Qualified Bidder 3 (Total Price – PKR)
Incl. all taxes
	Lowest Evaluated Bidder

	1
	BOQ–District Kech
	
	
	
	

	Lot No. 02

	Sr. No
	BOQ Reference
	Qualified Bidder 1 (Total Price – PKR) incl. all taxes
	Qualified Bidder 2 (Total Price – PKR)
Incl. all taxes
	Qualified Bidder 3 (Total Price – PKR)
Incl. all taxes
	Lowest Evaluated Bidder

	1
	BOQ–District Dera Bughti
	
	
	
	

	Lot No. 03

	Sr. No
	BOQ Reference
	Qualified Bidder 1 (Total Price – PKR) incl. all taxes
	Qualified Bidder 2 (Total Price – PKR)
Incl. all taxes
	Qualified Bidder 3 (Total Price – PKR)
Incl. all taxes
	Lowest Evaluated Bidder

	1
	BOQ– Gawadar
	
	
	
	

	Lot No. 04

	Sr. No
	BOQ Reference
	Qualified Bidder 1 (Total Price – PKR) incl. all taxes
	Qualified Bidder 2 (Total Price – PKR)
Incl. all taxes
	Qualified Bidder 3 (Total Price – PKR)
Incl. all taxes
	Lowest Evaluated Bidder

	1
	BOQ–District 
	
	
	
	

	Lot No. 05



Moreover;
i. Subsequently, the prepared Financial Evaluation Report shall duly be signed by all the members of the Procurement Committee.
ii. Comparatives of Financial will be prepared and signed by the procurement Committee in detail.
iii. If there is any discrepancy between Unit rate and total rate, the unit rate will always govern.
iv. If there is any discrepancy in tender documents clause and Work Order Clause, the work order Clause will always govern.
v. If there is any discrepancy between amount in words and amount in figures, the amount in words will always govern.

5. Recommendation of Procurement Committee 

I-      After Financial Evaluation (of only technically approved bidders), the contract will be awarded to the “Lowest Financially Evaluated bidder lotwise” with minimum quoted rates among all the Technical Qualified Bidders. 
II-      PPHI-Balochistan reserves the right to award complete work as per mentioned as detailed in data sheet of assignment of this document or partially as this shall be subject to availability of funds.







TERMS AND CONDITIONS:
1. Tenders must be quoted in Pakistani Rupees (PKR).
2. Tax Liability:
i. Complete Tax liability is to be borne by the Vendor/individual as per the applicable rate of tax authority.
ii. Quoted prices shall be inclusive of all applicable Taxes with maintaining of %age ofBRA/ GST.
iii. In-case of any Tax exemptions, exemption certificate from the concerned Tax Office / Regional Tax Office pertaining particularly to this case may be provided; otherwise, taxes shall be deducted as per Government Policy / Rules.
3. Bid Security of successful bidder/s shall be released after 30 days of completion of all deliveries as per work/supply order. 
4. The bid security of successful bidders submitted by the firm shall be considered as performance security. However, if the firm/vendor opts, a separate Bid Security amounting to 2% of the total work/supply order value in lieu of total bid security or performance Security.
5. Bid Security of unsuccessful bidder/s shall be released within 10 working days from the date of award of contract to the successful bidder/s.
6. Payment release is subject to 100% work completion duly signed by the authorized officials by competent authority PPHI-Balochistan.
7. Payment:
i. Advance payment is not allowed.

ii. Finance section will release 90% payment after completion of 100% work and 10% payment will be release after completion of 90 days of work completion period.

iii. Payment shall be made upon successful supply of 100% of the total ordered items. Payment for 50% of the supplied quantity will be processed, while 10% shall be withheld as performance security until completion of the remaining supplies. The balance payment will be released upon 100% successful delivery of the remaining items within 20 working days subject to the submission of all required documents and verification of quality as per the specifications outlined in the tender documents and approved samples.
CURRENCY & BID VALIDITY
· Pak Rupees & 90 Days













	[bookmark: Summary]  
	PEOPLE'S PRIMARY HEALTHCARE INITIATIVE BALOCHISTAN (PPHI-B)

	Summary of New Establishment of District Office & Major/Minor Works BHUs and DO 2026 

	Sr. No.
	 District Name
	Sr. No.
	BHU Name
	Estimated Amount

	01
	Kech
	1
	BHU KUNCHATTI
	1,595,311

	02
	Dera Bugti
	1
	BHU SHAMOLE
	2,301,192

	
	
	2
	BHU HABIB RAHI
	2,926,736

	
	
	3
	BHU JANI KHAN
	3,962,815

	
	
	4
	BHU MARROW
	2,680,173

	
	
	5
	BHU PEER KOH
	2,714,430

	
	
	6
	BHU PEETOKH
	1,632,243

	
	
	7
	BHU SERLOPE
	2,542,653

	
	
	8
	DO DERA BUGTI (ADDITIONAL WORK)
	3,946,003

	
	
	9
	WAREHOUSE
	2,332,928

	03
	Gawadar
	1
	BHU ZAHRAN
	1,072,546

	04
	Upper Dera Bughti
	1
	DISTRICT OFFICE
	4,177,819

	05
	Barshor
	2
	DISTRICT OFFICE
	3,847,791

	Total Amount
(Inclusive of: All Taxes, Labor cost & Transportation charges)
	35,732,640




[bookmark: BHU_Basti_Karim_Ishani_Barkhan]


DECLARATION BY THE BIDDER

	I solemnly undertake that:

a. Having read, understood & made myself aware of all the Terms & conditions mentioned in this Bidding Document & the Rules, Regulations & Policies of the Government of Balochistan, governing the procurement & financial matters, AGREE, ACCEPT & UNDETAKE TO ABIDE BY THE SAME.

b. The information provided in this form is correct to the best of my knowledge & in the event of change; details will be provided as soon as possible 

Name & Designation 							__________________ 

Signature 							Date 					

Company Stamp. ___________________________________________

















                                                                                                                             LOT  01
                                                    Sign and Stamp
                                          
	[bookmark: BHU_Kunchatti_Kech]BHU Kunchatti Repair and Renovation Work

	S.No
	DESCRIPTION
	Length
(L)
	Width
(W)
	Height
(H)
	QTY
	UNIT
	RATE
	AMOUNT

	1
	Dismantling of Roof
	
	
	
	
	
	
	

	
	Dismantling reinforced cement concrete, separating
reinforcement from concrete, clearing and straightening the
same
	
	
	
	
	
	
	

	
	Room-1
	16
	14.00
	0.5
	112
	
	
	

	
	Room-2
	16
	14.00
	0.5
	112
	
	
	

	
	Room-3
	16
	14.00
	0.5
	112
	
	
	

	
	Verandah
	10
	8.00
	0.5
	40
	
	
	

	
	
	
	
	
	376
	Cft
	
	

	2
	Girders & T iron
	
	
	
	
	
	
	

	
	Fabrication of heavy steel work with angle, tees, flat iron, round iron and sheet iron for making trusses, girders, tanks etc. including cutting, drilling riveting,handling,assembling and fixing but excluding erection in position as per
directions of Engineer
	
	
	
	
	
	
	

	
	Girders (22Nos)
	14
	3
	
	924
	
	
	

	
	T iron (75Nos)
	12
	0.5
	
	450
	
	
	

	
	
	
	
	
	1374
	kg
	
	

	3
	Roofing
	
	
	
	
	
	
	

	
	Providing and laying first class tile roof insulation comprising single layer of tiles12"x6"x1 1/2"grouted with cement sand mortar 1:3 laid over 2.5" thick cement concrete1:4:8 over glass wool /roof kool sheet wrapped in polythene sheet 300 gauge(0.03mm.)over a coat of PB-4 bitumen layer at the rate of 1.65 Kg./Sq.m.
	
	
	
	
	
	
	

	
	Room-1
	16
	14.00
	
	224
	
	
	

	
	Room-2
	16
	14.00
	
	224
	
	
	

	
	Room-3
	16
	14.00
	
	224
	
	
	

	
	Verandah
	10
	8.00
	
	80
	
	
	

	
	
	
	
	
	752
	Sft
	
	

	4
	Roof Screading
	
	
	
	
	
	
	

	
	Providing and laying 1:2:4 P.C.C roof screeding using crushed stone 3/4" (19mm) including formwork, consolidation, finishing and curing
3" (75mm) nominal thick P.C.C. roof
screeding
	
	
	
	
	
	
	

	
	Room-1
	16
	14.00
	0.25
	56
	
	
	

	
	Room-2
	16
	14.00
	0.25
	56
	
	
	

	
	Room-3
	16
	14.00
	0.25
	56
	
	
	

	
	Verandah
	10
	8.00
	0.25
	20
	
	
	

	
	
	
	
	
	188
	cft
	
	

	5
	Tilling
	
	
	
	
	
	
	

	
	Providing and laying 1/4" to 3/8" (6mm to 9mm) thick Glazed/ Matt tiles of
any colour and size in ground floor laid over 1" (25mm) thick cement sand
mortar base including jointing and washing the tiles with white cement
slurry of matching color by using color
pigment and curing.
	
	
	
	
	
	
	

	
	03 Rooms Floor Tilling
	15
	13.00
	
	585
	
	
	

	
	Verandah
	10
	8.00
	
	240
	
	
	

	
	
	
	
	
	825
	Sft
	
	

	6
	Distempering
	
	
	
	
	
	
	

	
	Distempering with Berger, ICI or equivalent synthetic polyvinyl emulsion finish of approved shade in two or more coats over and including the cost of priming coat including preparation of surface viz. dusting, sandpapering or rubbing with pumice
stone, filling cracks or holes, ifany, removing blisters or other imperfections at any height and any floor. (@ at least 2.20 Liter per 10 Sq.m
	
	
	
	
	
	
	

	
	Room-1
	15
	13.00
	10
	755
	
	
	

	
	Room-2
	15
	13.00
	10
	755
	
	
	

	
	Room-3
	15
	13.00
	10
	755
	
	
	

	
	Verandah
	10
	8.00
	10
	440
	
	
	

	
	
	
	
	
	2705
	Sft
	
	

	7
	Weather Coat
	
	
	
	
	
	
	

	
	Applying weather resistant paint coating (Three coats (@ at least 3.00 Liter per 10 Sq.m)such as ICI/ Berger or equivalent paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning, scaffolding and
removal of debris.
	
	
	
	
	
	
	

	
	Weather Coat complete building exterior
	150
	
	11
	1650
	
	
	

	
	
	
	
	
	1650
	Sft
	
	

	8
	LDPE Water Tank
	
	
	
	
	
	
	

	
	Providing and fixing LDPE overhead tank 500 gallon capacity double ply, blue/white manufactured by Marjan, Master or
equivalent on top of any floor
	
	
	
	
	
	
	

	
	
	
	
	
	1
	Each
	
	

	9
	PPRC Pipes
	
	
	
	
	
	
	

	
	Providing, laying, cutting, jointing, testing and disinfecting PPRC
pipes confirming to ISO 4427, PN-20, complete in all respects
with specials and valves etc. including all fittings, connnections
and jointing material
	
	
	
	
	
	
	

	
	
	
	
	
	100
	ft.
	
	

	10
	Underground Water Tank (UGWT)
	
	
	
	
	
	
	

	
	Circular underground water tank Dia 6' and
10' deep, complete in all respect.
	
	
	
	1
	job
	
	

	11
	Water Pumping Machine
	
	
	
	
	
	
	

	
	Dunki Pump 2900 RPM 2 HP
	
	
	
	1
	No
	
	

	
	Total Estimated Cost
	

	
	 BRA (Note)      
	

	
	Grand Total Amount (Inclusive of: All Taxes, Labour cost & Transportation charges) 
Note: BRA as per applicable percentage of 2nd schedule of Repair & Maintenance on payments other than Balochistan consolidated fund. 
	








LOT 3
	[bookmark: BHU_Shamole_Dera_Bugti_]Repair and Renovation Work estimates for BHU Shamole Dera Bugti

	S.No
	Description
	Length (L)
	Width (W)
	Hight (H)
	QTY
	Unit
	Rate
	Amount

	
	BHU Building
	
	
	
	
	
	
	

	1
	Plaster
	
	
	
	
	
	
	

	
	3/4 inch (9mm) Thick Cement plaster
1.3 using course send on walls and columns in basement plinth and ground floor including making ages, corners and curing.
	
	
	
	
	
	
	

	
	BHU Building Exterior
	210
	
	12
	2520
	
	
	

	
	BHU Building Interior
	14
	12
	11
	2926
	
	
	

	
	
	
	
	
	5446
	Sft
	
	

	2
	Flooring
	
	
	
	
	
	
	

	
	Providing and laying Plain machine mixed 1:3:6 concrete using course send and crushed aggregate having maximum size upto 1/1.2’’(38 mm) and down guage in foundation including leveling , compacting and curing.
	
	
	
	
	
	
	

	
	Complete BHU Building interior rooms washrooms, veranda
flooring.
	
	
	
	
	
	
	

	
	
	14
	12
	0.5
	319
	cft
	
	

	3
	Roof Chemical treatment
	
	
	
	
	
	
	

	
	Providing and laying chemical
treatment on existing slabs for seapage protection.
	
	
	
	
1200
	
Sft
	
	

	4
	Under Ground Water Tank
	
	
	
	
	
	
	

	
	Circular underground water tank ‘’
10 x 10’’ and ‘’ 8 ‘’deep complete in all respect.
	
	
	
	
	
	
	

	
	
	
	
	
	1
	job
	
	

	5
	LDPE Water Tank
	
	
	
	
	
	
	

	
	Providing and fixing LDPE Over Head tank 500 gallon capacity double ply, blue/white manufactured by Marjan, Master or equivalent on top of any floor.
	
	
	
	
	
	
	

	
	
	
	
	
	1
	Each
	
	

	6
	Distempering
	
	
	
	
	
	
	

	
	Distempering with Berger, ICI or equivalent synthetic polyvinyl emulsion finish of approved shade in two or more coats over and including preparation of surface viz dusting sendpapering or rubbing with pumice
	
	
	
	
	
	
	

	
	Stone filling, cracks or holes if any removing blisters or other imperfections at any height and any floor (@ at least 2.20 Liter per
10 Sq.m
	
	
	
	
	
	
	

	
	Room -1 (BHU Building)
	14
	12
	11
	740
	
	
	

	
	Room -2 (BHU Building)
	14
	12
	11
	740
	
	
	

	
	Room -3 (BHU Building)
	14
	12
	11
	740
	
	
	

	
	
	
	
	
	
	
	
	

	
	Washroom-1
	6
	5
	11
	272
	
	
	

	
	
	
	
	
	
	
	
	

	
	Varandah (BHU Building)
	14
	7
	11
	406
	
	
	

	
	
	
	
	
	2898
	Sft
	
	

	7
	Weather Coat
	
	
	
	
	
	
	

	
	
Applying Weather resistant paint coating (Three Coats @ at Least 3.0 liter per 10 Sq.m) such as ICI, berger, or equivalent part of approved shade on old suface of walls and ceiling including dusting send papering and cleaning , scaffolding and removal of debris.
	
	
	
	
	
	
	

	
	BHU Building exterior
	210
	
	12
	2520
	
	
	

	
	
	
	
	
	2520
	Sft
	
	

	8
	Tilling
	
	
	
	
	
	
	

	
	Providing and lying 1.4’’ and 3.9’’ (6mm to 9mm) thick Gizared mat tiles of any color and sizes in ground floor laid over 1’’ (25mm) thick cement send mortar base including jointing and washing the tiles with white cement.
	
	
	
	
	
	
	

	
	Slurry of matching color by using
color pigment and curing.
	
	
	
	
	
	
	

	
	Washroom-1
	6
	6
	6
	180
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	180
	Sft
	
	

	9
	Door Installation
	
	
	
	
	
	
	

	
	Providing and fixing fully glazed Steel door with frame single leaf with M.S bottom or kick rail 6’’ (150mm) wide and top rail of 4’’ (100mm) wide painted with two coats with red oxide paint, brass oxidized fitting of lugs, cutting holed and making good the damages to walls
	
	
	
	
	
	
	

	
	
	
	
	
	120
	Sft
	
	

	10
	Window Installation
	
	
	
	
	
	
	

	
	Providing and fixing hot dipped galvanized fully glazed double leaf hung steel windows and ventilators of approved section with Z section 1.25* (32mm) width at each edge including using approved brass sections oxidized fitting, iron lugs. Cutting holes and making good the damages to wallas.
	
	
	
	
	
	
	

	
	Windows type- A
	4
	4
	
	48
	
	
	

	
	
	
	
	
	48
	Sft
	
	

	11
	Ceilling Fans
	
	
	
	4
	Each
	
	

	12
	Wiring
	
	
	
	
	
	
	

	
	Concealed/ open wiring from joint to switch with length upto 30ft. (10m)including any switch to switch wiring with 3x 1.5 sq.mm. PVC insulated single core copper conductor, Pakistan Cables, pioneer, newage or approved equivalent cables
	
	
	
	
	
	
	

	
	
	
	
	
	30
	Points
	
	

	13
	PPRC Pipe
	
	
	
	
	
	
	

	
	Providing laying cutting, jointing, testing and disinfecting PPRC pipe PN20 (32mm) Outer dia conforming to ISO 4427. PN20 complete in all respects with specials and valves etc. including all fitting, connections and jointing materials.
	
	
	
	
	
	
	

	
	
	
	
	
	200
	ft
	
	

	14
	Wash Basins
	
	
	
	
	
	
	

	
	Providing and fixing approved
quality fixtures wash basins 24’’ (610mm) ICL future make.
	
	
	
	
	
	
	

	
	
	
	
	
	1
	No.
	
	

	15
	Water Closet
	
	
	
	
	
	
	

	
	
Providing and fixing white English
W.C with glazed earthen were 4’’ (100mm) trap squatting type water closet with integral treads ICL Boch/ Karam Cera or approved equivalent make including cost of inlet pipe cistern and lid cistern kit, stop cock deluxe type and other accessories fitting brackets, PVC down pipe, rubbed rings/ washers, making requisites numbers of holes in walls, plinth and floor for pipe connection and making good with approved material.
	
	
	
	
	
	
	

	
	
	
	
	
	1
	Each
	
	

	16
	UPVC Sewerage pipe
	
	
	
	
	
	
	

	
	Providing and installing UPVC pipe class b having 4’’ (100mm inner dia) IIL, Dedax or equivalent make registered with PSQCA in sewer lines and/ or laying cutting, jointing, testing including all specials in pipe lines in trenches.
	
	
	
	
	
	
	

	
	
	
	
	
	40
	Rft
	
	

	17
	Soak Pit
	
	
	
	
	
	
	

	
	Providing and construction of soak pit having diameter 3’ with depth. Inner filled with bricks, ballast/ stone, ballast having RCC top, complete in all respects as per drawing and as per direction of Engineer.
	
	
	
	
	
	
	

	
	
	
	
	
	1
	No
	
	

	18
	Water Pumping Machine
	
	
	
	
	
	
	

	
	Dunki Pump 2900 RPM 2 HP
	
	
	
	1
	No
	
	

	19
	Washroom Accessories Set
	
	
	
	2
	Each
	
	

	20
	Sign Board and Direction Board
	
	
	
	
	
	
	

	
	Installation and fixation of Sign board 4x2 and direction board 4x4.
	
	
	
	
1
	
job
	
	

	21
	Main entrance door installation
(3x7) steel door.
	
	
	
	1
	job
	
	

	

22
	Miscellaneous works (Complete BHU Ground leveling and filling by crush stone neec base, glass repair, window mesh repair, door locks, plumbing repair etc)
	
	
	
	

1
	

job
	
	

	23
	Dust bin 3 and Visal charts (12)
	
	
	
	3
	set
	
	

	
	Total Estimated Cost
	

	
	 BRA (Note)      
	

	
	Grand Total Amount (Inclusive of: All Taxes, Labour cost & Transportation charges) 
Note: BRA as per applicable percentage of 2nd schedule of Repair & Maintenance on payments other than Balochistan consolidated fund. 
	



	
[bookmark: BHU_Habib_Rahi_Dera_Bugti]DETAILED ESTIMATE FOR REHABILITATION BASIC HEALTH UNIT HABIB RAHI DERA BUGTI

	S. No
	Description of work
	No.
	Measurement
	Quantity
	Unit
	Rate
	Amount

	
	
	
	Length
	Width
	Height
	
	
	
	

	
1
	Dismantling reinforced cement concrete, separating reinforcement from concrete,
clearing and straightening the same
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	14.00
	12.00
	0.50
	420.00
	cft
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	10.00
	0.50
	40.00
	cft
	
	
	

	
	Bath
	1
	x
	2
	6.00
	6.00
	0.50
	36.00
	cft
	
	
	

	
	
	
	
	
	
	
	
	496.00
	cft
	
	
	

	
2
	Providing rolled steel joists and channels including hoisting and fixing in position in cement concrete but excluding the cost of
cement concrete
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	14.00
	4
	
	280.00
	kgs
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	4
	
	32.00
	kgs
	
	
	

	
	Bath
	1
	x
	2
	6.00
	4
	
	48.00
	kgs
	
	
	

	
	
	
	
	
	
	
	
	360.00
	
	
	
	

	3
	Providing M.S. Tees, angles and flats
including fixing in position.
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	14.00
	12.00
	1.50
	1260.00
	lbs
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	10.00
	1.50
	120.00
	lbs
	
	
	

	
	Bath
	1
	x
	2
	6.00
	6.00
	1.50
	108.00
	lbs
	
	
	

	
	
	
	
	
	
	
	
	1488.00
	lbs
	
	
	

	
	
	
	
	1488/2.204
	
	
	675.14
	kg
	
	
	

	




4
	Providing and laying second class brick tile roofing comprising 4 inches (100mm) thick earth and 1 inch (25 mm) thick mud plaster with gobri leeping over 1/2 inch (13mm) thick cement plaster 1:6 with 34 lbs./100 Sq.ft.(1.65 Kg./Sq.m.) hot bitumen coating sand blended in one coat, provided over one layer of tiles 12" x 6"x 2" laid in 1:6 cement sand mortar including 1:2 cement sand pointing underside of tiles including curing
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	15.50
	13.50
	
	1046.25
	Sft
	
	
	

	
	Verendah
	1
	x
	1
	9.50
	11.50
	
	109.25
	Sft
	
	
	

	
	Bath
	1
	x
	2
	7.50
	7.50
	
	112.50
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	1268.00
	Sft
	
	
	

	




5
	Providing and laying 1:2:4 P.C.C roof screeding using crushed stone 3/4" (19mm) including formwork, consolidation, finishing and curing. 1-1/2" (37.5mm) nominal thick
P.C.C. roof screeding
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	15.50
	13.50
	
	1046.25
	Sft
	
	
	

	
	Verendah
	1
	x
	1
	9.50
	11.50
	
	109.25
	Sft
	
	
	

	
	Bath
	1
	x
	2
	7.50
	7.50
	
	112.50
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Total
	1268.00
	Sft
	
	
	

	6
	Scraping, rubbing and cleaning of oil bound distemper
	
	
	
	
	
	
	
	

	
	Ceiling
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	15.50
	13.50
	
	1046.25
	Sft
	
	
	

	
	Verendah
	1
	x
	1
	9.50
	11.50
	
	109.25
	Sft
	
	
	

	
	Bath
	1
	x
	2
	7.50
	7.50
	
	112.50
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Walls
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	4
	x
	5
	15.50
	
	12.00
	3720.00
	Sft
	
	
	

	
	Verendah
	4
	x
	1
	9.50
	
	12.00
	456.00
	Sft
	
	
	

	
	Bath
	4
	x
	2
	7.50
	
	12.00
	720.00
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	TOTAL
	6164.00
	
	
	
	

	
	Projection
	1
	x
	1
	120.00
	2.50
	
	300.00
	Sft
	
	
	

	
	
	
	
	
	
	Sub Total
	6464.00
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	5
	x
	1
	3.50
	
	6.50
	113.75
	Sft
	
	
	

	
	D2
	2
	x
	1
	2.50
	
	6.50
	32.50
	Sft
	
	
	

	
	W1
	5
	x
	1
	4
	
	5.00
	100.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	246.25
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Net Qty.
	6217.75
	Sft
	
	
	

	7
	Distempering with Berger/ ICI or equivalent synthetic
	
	
	
	
	
	
	
	

	
	Ceiling and Internal walls Quantity
	1
	x
	2
	6164.0
	
	Net Qty.
	12328.00
	Sft
	
	
	

	8
	Painting old surface in ground floor or basement with
	
	
	
	
	
	
	
	

	
	Qty of Door and Windows
	1
	x
	2
	
	
	Net Qty.
	246.25
	Sft
	
	
	

	

9
	1/2 inch ( 13mm) thick cement plaster using Coarse Sand on wall sand columns in basement, plinth and ground floor including making edges, corners and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	6464.0
	
	
	6464.00
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	5
	x
	1
	3.50
	
	6.50
	113.75
	Sft
	
	
	

	
	D2
	2
	x
	1
	2.50
	
	6.50
	32.50
	Sft
	
	
	

	
	W1
	5
	x
	1
	4.00
	
	5.00
	100.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	246.25
	Sft
	
	
	

	
	
	
	
	
	
	
	Net Total
	4217.75
	Sft
	
	
	

	

10
	Providing and laying 1:4:8 hand mixed cement concrete bed under floors using graded shingle or bajri 50 mm and down guage complete with levelling ramming
watering and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	15.50
	13.50
	0.25
	261.56
	cft
	
	
	

	
	Verendah
	1
	x
	1
	9.50
	11.50
	0.25
	27.31
	cft
	
	
	

	
	Bath
	1
	x
	2
	7.50
	7.50
	0.25
	28.13
	cft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	317.00
	cft
	
	
	

	

11
	Providing and fixing 1/4" to 3/8" (6mm to 9mm) thick
	
	
	
	
	
	
	
	

	
	Bath
	1
	x
	1
	23.00
	
	7.00
	161.00
	sft
	
	
	

	
	Deduction
	
	
	
	
	
	Total
	161.00
	sft
	
	
	

	
	d1
	1
	x
	1
	2.50
	
	6.50
	16.25
	sft
	
	
	

	
	
	
	
	
	
	
	Total
	16.25
	sft
	
	
	

	
	
	
	
	
	
	
	Net Qty
	144.75
	sft
	
	
	

	
12
	Providing and laying 1/4" to 3/8" (6mm to 9mm) thick
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	15.50
	13.50
	
	1046.25
	sft
	
	
	

	
	Verendah
	1
	x
	1
	9.50
	11.50
	
	109.25
	sft
	
	
	

	
	Bath
	1
	x
	2
	7.50
	7.50
	
	112.50
	sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	1268.00
	sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	ELECTRICAL WORK
	
	
	
	
	
	
	
	
	
	
	

	13
	Concealed wiring from point to switch with 3/4" (20
	
	
	
	
	
	
	
	

	
	
	10
	x
	1
	
	
	
	10.00
	Point
	
	
	

	14
	Concealed wiring for 5 Amp. Socket outlets from
	
	
	
	
	
	
	
	

	
	
	12
	x
	1
	
	
	
	12.00
	Point
	
	
	

	15
	Supply and install 2-gang, 5 Amp, 250 Volt,. plate type
	
	
	
	
	
	
	
	

	
	
	12
	x
	1
	
	
	
	12.00
	No.
	
	
	

	16
	Supply and install combined 2/3 pin 5 Amps, 250 Volt
	
	
	
	
	
	
	
	

	
	
	12
	x
	1
	
	
	
	12.00
	No.
	
	
	

	
17
	Supply and install Energy Saver electric
bulbs
	
	
	
	
	
	
	
	
	
	
	

	
	
	26
	x
	1
	
	
	
	26.00
	No.
	
	
	

	18
	Supply and install 10" (250 mm) sweep exhaust fan
	
	
	
	
	
	
	
	

	
	
	6
	x
	1
	
	
	
	6.00
	No.
	
	
	

	19
	Installing each number circuit breaker 6 Ampere on same
	
	
	
	
	
	
	
	

	
	
	1
	x
	2
	
	
	
	2.00
	No.
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Boundary Wall Work
	
	
	
	
	
	
	
	
	
	
	

	
20
	3/4 inch (19mm) thick cement plaster 1:4 using Coarse
	
	
	
	
	
	
	
	

	
	Walls
	2
	x
	4
	40.00
	
	7.75
	2480.00
	sft
	
	
	

	
	
	
	
	
	
	
	Total
	2480.00
	sft
	
	
	

	
21
	Applying weather resistant paint coating such as ICI
	
	
	
	
	
	
	
	

	
	Walls
	1
	x
	4
	40.00
	
	7.75
	1240.00
	sft
	
	
	

	
	
	
	
	
	
	
	Total
	1240.00
	sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Tuff Tile Work
	
	
	
	
	
	
	
	
	
	
	

	22
	Earthwork for embankment lead upto 100 ft. (30m) and compaction by Manual (Maximium Area 250 Sft) labour at optimum moisture content, dressing to designed section, laying,
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	
	100
	x
	10
	1000
	Cft
	
	
	

	
	
	
	
	
	
	
	
	1000
	Cft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	23
	Supply and Fixing of Concrete pavers on sand cushion of different designs having thickness of 60 mm, mechnically compressed, minimium strenght of 4500 psi after laboratory testing at factory and random testiing at site as and when desired by the Engineer inchange comple in all respects.
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	
	100
	x
	10
	1000
	Sft
	
	
	

	
	
	
	
	
	Total
	
	
	1000
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	24
	Providing and laying plain machine mixed cement concrete using coarse sand and crushed aggregate having maximum size upto 11/2" (38mm) & down gauge in foundation including levelling, compacting
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	2
	x
	
	100
	0.5
	0.25
	25
	Cft
	
	
	

	
	
	
	
	
	
	
	
	25
	Cft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Total Estimated Cost
	

	
	 BRA (Note)      
	

	
	Grand Total Amount (Inclusive of: All Taxes, Labour cost & Transportation charges) 
Note: BRA as per applicable percentage of 2nd schedule of Repair & Maintenance on payments other than Balochistan consolidated fund. 
	














	[bookmark: BHU_Jani_Khan]DETAILED ESTIMATE FOR REHABILITATION BASIC HEALTH UNIT JANI KHAN DISTRICT DERA BUGTI

	

	S.No
	Description of work
	No.
	Measurement
	Quantity
	Unit
	Rate
	Amount

	
	
	
	Length
	Width
	Height
	
	
	
	

	



1
	Providing and laying 1:2:4 P.C.C roof screeding using crushed stone 3/4" (19mm) including formwork, consolidation, finishing and curing. 1-1/2" (37.5mm) nominal thick P.C.C. roof screeding
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	4
	14.00
	14.00
	
	784.00
	Sft
	
	
	

	
	Verendah
	1
	x
	1
	10.00
	8.00
	
	80.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	864.00
	Sft
	
	
	

	
2
	Scraping, rubbing and cleaning of oil bound distemper from ceiling and walls including removal of rubbish in ground floor
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	4
	14.00
	14.00
	
	784.00
	Sft
	
	
	

	
	Verendah
	1
	x
	1
	10.00
	8.00
	
	80.00
	Sft
	
	
	

	
	Walls
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	2
	x
	4
	28.00
	
	12.00
	2688.00
	Sft
	
	
	

	
	
	2
	x
	1
	18.00
	
	12.00
	432.00
	Sft
	
	
	

	
	
	
	
	
	
	
	TOTAL
	3984.00
	
	
	
	

	
	Projection
	1
	x
	1
	120.00
	2.50
	
	300.00
	Sft
	
	
	

	
	
	
	
	
	
	Sub Total
	4284.00
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	4
	x
	1
	3.50
	
	6.50
	91.00
	Sft
	
	
	

	
	D2
	2
	x
	1
	2.50
	
	6.50
	32.50
	Sft
	
	
	

	
	W1
	4
	x
	1
	4
	
	5.00
	80.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	203.50
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Net Qty.
	4080.50
	Sft
	
	
	

	


3
	Distempering with Berger/ ICI or equivalent synthetic vinyl emulsion paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning in ground floor.
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling and Internal walls Quantity
	1
	x
	2
	3984.0
	
	Net Qty.
	7968.00
	Sft
	
	
	

	
4
	Painting old surface in ground floor or basement with
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Qty of Door and Windows
	1
	x
	2
	
	
	Net Qty.
	203.50
	Sft
	
	
	

	
5
	1/2 inch ( 13mm) thick cement plaster using Coarse Sand on wall sand columns in basement, plinth and ground floor including making edges,
corners and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	4284.0
	
	
	4284.00
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	4
	x
	1
	3.50
	
	6.50
	91.00
	Sft
	
	
	

	
	D2
	2
	x
	1
	2.50
	
	6.50
	32.50
	Sft
	
	
	

	
	W1
	4
	x
	1
	4.00
	
	5.00
	80.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	203.50
	Sft
	
	
	

	
	
	
	
	
	
	
	Net Total
	4080.50
	Sft
	
	
	

	

6
	Providing and laying 1:4:8 hand mixed cement concrete bed under floors using graded shingle or bajri 50 mm and down guage complete with levelling ramming watering and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	2
	14.00
	14.00
	0.25
	98.00
	cft
	
	
	

	
	
	1
	x
	1
	10.00
	8.00
	0.25
	20.00
	cft
	
	
	

	
	
	
	
	
	
	
	
	177.00
	cft
	
	
	

	



7
	Providing and laying 1/4" to 3/8" (6mm to 9mm) thick Glazed/ Matt tiles of any colour and size in ground floor laid over 1" (25mm) thick cement sand mortar base including jointing and washing the tiles with white cement slurry of matching color by using color pigment and curing
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	1
	14.00
	14.00
	
	266.00
	cft
	
	
	

	
	
	
	
	
	
	
	
	266.00
	sft
	
	
	

	
	Plumbing
	
	
	
	
	
	
	
	
	
	
	

	




8
	Providing and fixing squatting type water closet with integral treads ICL Boch/Karam Cera or approved equivalent make including cost of inlet pipe cistern and lid cistern kit, stop cock deluxe type and other accessories, fittings, brackets, PVC down pipe, rubber rings/washers.
	
	
	
	
	
	
	
	

	
	
	
1
	
x
	
1
	
	
	
	
1.00
	
No
	
	
	

	

9
	Providing and fixing export quality glazed earthen ware wash basin manufactured by ICL Boch/Karam Cera or equivalent approved make with single hole chromium plated mixer tap
1/2" (15mm), pillar tap delux, stop cocks, C.I. or W.I.
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	
	
	
	1.00
	No
	
	
	

	

10
	Providing, laying, cutting, jointing, testing and disinfecting PVC pipes confirming to BSS-3505/PS-3051 complete in all respects.
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	
	
	
	300.00
	Rft
	
	
	

	


11
	Providing, laying, cutting, jointing, testing and disinfecting PPRC pipes (25mm) confirming to ISO 4427, PN-20, complete in all respects with specials and valves etc. including all fittings, connnections and jointing material
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	300.00
	
	Total
	300.00
	Rft
	
	
	

	

12
	Providing and fixing C.P brass shower having 1/2" (12 mm) dia inlet and 6" (150 mm) dia. detachable lid
	
	
	
	
	
	
	
	

	
	
	1
	x
	2
	
	
	
	2.00
	Each
	
	
	

	

13
	Providing and fixing superior quality C.P. bib cock of approved make. 1/2" (12 mm) dia.
	
	
	
	
	
	
	
	

	
	
	1
	x
	6
	
	
	
	6.00
	Each
	
	
	

	

14
	Providing and fixing Cement concrete gulley trap 6" x 6" x 4" (150 x 150 x 100 mm) with C.I. cover and frame weighing not less than 10 kg.
	
	
	
	
	
	
	
	

	
	
	1
	x
	6
	
	
	Total
	6.00
	No
	
	
	

	
15
	Providing and fixing approved quality chromium plated towel
rail with bracket and screws.
	
	
	
	
	
	
	
	

	
	
	1
	x
	4
	
	
	
	4.00
	No.
	
	
	

	
16
	Providing and fixing approved quality C.P. brass toilet paper holder Master /Sonex or equivalent make.
	
	
	
	
	
	
	
	

	
	
	1
	x
	4
	
	
	
	4.00
	No.
	
	
	

	

17
	Providing and fixing looking mirror of Belgium/ Malaysian/ Indonesian glass with chromium plated screws.
	
	
	
	
	
	
	
	

	
	
	1
	x
	2
	
	
	2.00
	4.00
	sft
	
	
	

	
18
	Providing and fixing soap dish Chromium plated.
	
	
	
	
	
	
	
	

	
	
	1
	x
	2
	
	
	
	2.00
	No.
	
	
	

	
19
	Providing and fixing 'P' trap including concrete chamber and
C.I. grating Glazed 4" (100 mm) size.
	
	
	
	
	
	
	
	

	
	
	1
	x
	6
	
	
	
	6.00
	No
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	CONSTRUCTION OF BOUNDARY WALL

	20
	Excavation in foundation of buildings including layout,
	
	
	
	
	
	
	
	

	
	
	4
	x
	1
	80.00
	2.00
	2.50
	1600.00
	cft
	
	
	

	21
	Providing and laying cement concrete using approved
	
	
	
	
	
	
	
	

	
	
	4
	x
	1
	80.00
	2.00
	0.25
	160.00
	cft
	
	
	

	

22
	Providing and laying 1:4:8 cement concrete block masonry
	
	
	
	
	
	
	
	

	
	1st step
	4
	x
	1
	80.000
	1.87
	0.75
	448.80
	cft
	
	
	

	
	2nd step
	4
	x
	1
	79.625
	1.5
	1.00
	477.75
	cft
	
	
	

	
	3rd step
	4
	x
	1
	79.375
	1.125
	1.25
	446.48
	cft
	
	
	

	
	
	
	
	
	
	
	Total
	1373.03
	cft
	
	
	

	
23
	Providing and laying 1:4:8 cement concrete block masonry
	
	
	
	
	
	
	
	

	
	Wall
	1
	x
	1
	80.00
	1
	6.00
	480.00
	cft
	
	
	

	
	
	
	
	
	
	
	Net
	480.00
	cft
	
	
	

	24
	Providing and laying 1:2:4 cement concrete using approved
	
	
	
	
	
	
	
	

	
	Coping
	1
	x
	1
	80.00
	1
	0.25
	20.00
	cft
	
	
	

	
	3/4 inch (19mm) thick cement plaster 1:4 using Coarse
	
	
	
	
	
	
	
	

	25
	Walls
	2
	x
	4
	80.00
	
	7.75
	4960.00
	sft
	
	
	

	
	
	
	
	
	
	
	Total
	4960.00
	sft
	
	
	

	
26
	Providing and fixing collapsible steel shutter or gate
	
	
	
	
	
	
	
	

	
	Gate
	1
	x
	1
	10.00
	
	8.00
	80.00
	sft
	
	
	

	
	
	
	
	
	
	
	Total
	80.00
	sft
	
	
	

	
27
	Applying weather resistant paint coating such as ICI
	
	
	
	
	
	
	
	

	
	Walls
	1
	x
	4
	80.00
	
	7.75
	2480.00
	sft
	
	
	

	
	
	
	
	
	
	
	Total
	2480.00
	sft
	
	
	

	
28
	Painting with ICI/Berger or equivalent super gloss
	
	
	
	
	
	
	
	

	
	Gate
	1
	x
	2
	10.00
	
	8.00
	20.00
	sft
	
	
	

	
	
	
	
	
	
	
	Total
	20.00
	sft
	
	
	

	Bathroom Repair/Rehablitation work (02 Nos)

	29
	Providing rolled steel joists and channels including
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Bath
	2
	x
	1
	6.00
	6
	
	72.00
	kgs
	
	
	

	
	
	
	
	
	
	
	
	72.00
	
	
	
	

	30
	Providing M.S. Tees, angles and flats including
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Bath
	2
	x
	1
	6.00
	6.00
	1.50
	108.00
	lbs
	
	
	

	
	
	
	
	
	
	
	
	108.00
	lbs
	
	
	

	
	
	
	
	5406/2.204
	
	
	49.00
	kg
	
	
	

	31
	Providing and laying second class brick tile
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Bath
	2
	x
	1
	7.50
	7.50
	
	112.50
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	112.50
	Sft
	
	
	

	
32
	Providing and laying 1:2:4 P.C.C roof screeding using
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Bath
	2
	x
	1
	7.50
	7.50
	
	112.50
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	112.50
	Sft
	
	
	

	33
	Scraping, rubbing and cleaning of oil bound distemper from
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling
	
	
	
	
	
	
	
	
	
	
	

	
	Bath
	2
	x
	1
	7.50
	7.50
	
	112.50
	Sft
	
	
	

	
	Walls
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	2
	x
	4
	15.00
	
	12.00
	1440.00
	Sft
	
	
	

	
	
	
	
	
	
	
	TOTAL
	1552.50
	
	
	
	

	
	Projection
	1
	x
	1
	120.00
	2.50
	
	300.00
	Sft
	
	
	

	
	
	
	
	
	
	Sub Total
	1852.50
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	2
	x
	1
	3.50
	
	6.50
	45.50
	Sft
	
	
	

	
	D2
	2
	x
	1
	2.50
	
	6.50
	32.50
	Sft
	
	
	

	
	V
	2
	x
	1
	2
	
	2.00
	8.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	86.00
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Net Qty.
	1766.50
	Sft
	
	
	

	
34
	Distempering with Berger/ ICI or equivalent synthetic vinyl
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling and Internal walls Quantity
	1
	x
	2
	1552.5
	
	Net Qty.
	3105.00
	Sft
	
	
	

	
35
	Painting old surface in ground floor or basement with
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Qty of Door and Windows
	1
	x
	2
	
	
	Net Qty.
	86.00
	Sft
	
	
	

	36
	1/2 inch ( 13mm) thick cement plaster using
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	1852.5
	
	
	1852.50
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	2
	x
	1
	3.50
	
	6.50
	45.50
	Sft
	
	
	

	
	D2
	2
	x
	1
	2.50
	
	6.50
	32.50
	Sft
	
	
	

	
	V
	2
	x
	1
	2.00
	
	2.00
	8.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	86.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Net Total
	1766.50
	Sft
	
	
	

	37
	Providing and laying 1:4:8 hand mixed cement
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	6.00
	6.00
	0.25
	9.00
	cft
	
	
	

	
	
	
	
	
	
	
	
	13.50
	cft
	
	
	

	

38
	Providing and fixing 1/4" to 3/8" (6mm to 9mm) thick
	
	
	
	
	
	
	
	

	
	Bath
	2
	x
	4
	6.00
	
	7.00
	336.00
	sft
	
	
	

	
	Deduction
	
	
	
	
	
	Total
	436.80
	sft
	
	
	

	
	d1
	2
	x
	1
	2.50
	
	6.50
	32.50
	sft
	
	
	

	
	
	
	
	
	
	
	Total
	32.50
	sft
	
	
	

	
	
	
	
	
	
	
	Net Qty
	404.30
	sft
	
	
	

	39
	Providing and laying 1/4" to 3/8" (6mm to 9mm) thick
	
	
	
	
	
	
	
	

	
	Bath
	2
	x
	1
	6.00
	6.00
	
	228.00
	cft
	
	
	

	
	
	
	
	
	
	
	
	228.00
	sft
	
	
	

	
	ELECTRICAL WORK
	
	
	
	
	
	
	
	
	
	
	

	40
	Concealed wiring from point to switch with 3/4" (20
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	
	
	
	1.00
	Point
	
	
	

	41
	Concealed wiring for 5 Amp. Socket outlets from
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	
	
	
	1.00
	Point
	
	
	

	42
	Supply and install 2-gang, 5 Amp, 250 Volt,. plate type
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	
	
	
	1.00
	No.
	
	
	

	43
	Supply and install combined 2/3 pin 5 Amps, 250 Volt
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	
	
	
	1.00
	No.
	
	
	

	44
	Supply and install Energy Saver electric bulbs
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	
	
	
	1.00
	No.
	
	
	

	45
	Supply and install 10" (250 mm) sweep exhaust fan
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	
	
	
	1.00
	No.
	
	
	

	46
	Installing each number circuit breaker 6 Ampere on same
	
	
	
	
	
	
	
	

	
	
	1
	x
	2
	
	
	
	2.00
	No.
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	Tuff Tiles Work

	1.
	Earthwork for embankment lead upto 100 ft. (30m) and compaction by Manual (Maximium Area 250 Sft) labour at optimum moisture content,
dressing to designed section, laying, leveling and
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	
	120
	10
	=
	1200
	Cft
	
	
	

	
	
	
	
	
	
	
	
	1200
	Cft
	
	
	

	
	
	
	
	
	
	
	
	
	@
	
	
	

	2
	Supply and Fixing of Concrete pavers on sand cushion of different designs having thickness of
60 mm, mechnically compressed, minimium strenght of 4500 psi after laboratory testing at factory and random testiing at site as and when desired by the Engineer inchange comple in all
respects. (No PCC work is premitted underneath
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	
	120
	10
	=
	1200
	Sft
	
	
	

	
	
	
	
	
	
	
	
	1200
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	@
	
	
	

	3
	Providing and laying plain machine mixed cement concrete using coarse sand and crushed aggregate having maximum size upto 11/2" (38mm) & down gauge in foundation including
levelling, compacting and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	2
	x
	
	120
	0.5
	0.25
	30
	Cft
	
	
	

	
	
	
	
	
	
	
	
	30
	Cft
	
	
	

	
	
	
	
	
	
	
	
	
	Rs.
	
	
	

	
	Total Estimated Cost
	

	
	 BRA (Note)      
	

	
	Grand Total Amount (Inclusive of: All Taxes, Labour cost & Transportation charges) 
Note: BRA as per applicable percentage of 2nd schedule of Repair & Maintenance on payments other than Balochistan consolidated fund. 
	



[bookmark: BHU_Marrow]
	DETAILED ESTIMATE FOR REHABILITATION BASIC HEALTH UNIT SERLOPE MARROW DERA BUGTI

	

	S.No
	Description of work
	No.
	Measurement
	Quantity
	Unit
	Rate
	Amount

	
	
	
	Length
	Width
	Height
	
	
	
	

	
1
	Dismantling reinforced cement concrete, separating reinforcement from concrete,
clearing and straightening the same
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	14.00
	14.00
	0.50
	490.00
	cft
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	12.00
	0.50
	48.00
	cft
	
	
	

	
	Bath
	1
	x
	2
	7.00
	7.00
	0.50
	49.00
	cft
	
	
	

	
	
	
	
	
	
	
	
	587.00
	cft
	207.62
	
	

	
2
	Providing rolled steel joists and channels including hoisting and fixing in position in cement concrete but excluding the cost of
cement concrete
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	14.00
	4
	
	280.00
	kgs
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	4
	
	32.00
	kgs
	
	
	

	
	Bath
	1
	x
	2
	7.00
	4
	
	56.00
	kgs
	
	
	

	
	
	
	
	
	
	
	
	368.00
	
	394.18
	
	

	3
	Providing M.S. Tees, angles and flats including
fixing in position.
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	14.00
	14.00
	1.50
	1470.00
	lbs
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	12.00
	1.50
	144.00
	lbs
	
	
	

	
	Bath
	1
	x
	2
	7.00
	7.00
	1.50
	147.00
	lbs
	
	
	

	
	
	
	
	
	
	
	
	1761.00
	lbs
	
	
	

	
	
	
	
	5406/2.204
	
	
	799.00
	kg
	406.97
	
	

	




4
	Providing and laying second class brick tile roofing comprising 4 inches (100mm) thick earth and 1 inch (25 mm) thick mud plaster with gobri leeping over 1/2 inch (13mm) thick cement plaster 1:6 with 34 lbs./100 Sq.ft.(1.65 Kg./Sq.m.) hot bitumen coating sand blended in one coat, provided over one layer of tiles 12" x 6"x 2" laid in 1:6 cement sand mortar including 1:2 cement sand pointing underside of tiles including curing
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	14.00
	14.00
	
	980.00
	Sft
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	12.00
	
	96.00
	Sft
	
	
	

	
	Bath
	1
	x
	2
	7.00
	7.00
	
	98.00
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	1174.00
	Sft
	204.82
	
	

	




5
	Providing and laying 1:2:4 P.C.C roof screeding using crushed stone 3/4" (19mm) including formwork, consolidation, finishing and curing. 1-1/2" (37.5mm) nominal thick P.C.C. roof screeding
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	15.50
	15.50
	
	1201.25
	Sft
	
	
	

	
	Verendah
	1
	x
	1
	9.50
	13.50
	
	128.25
	Sft
	
	
	

	
	Bath
	1
	x
	2
	8.50
	8.50
	
	144.50
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Total
	1474.00
	Sft
	121.40
	P.Sft
	

	
6
	Scraping, rubbing and cleaning of oil bound distemper from ceiling and walls including removal of rubbish in ground floor
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	15.50
	15.50
	
	1201.25
	Sft
	
	
	

	
	Verendah
	1
	x
	1
	9.50
	13.50
	
	128.25
	Sft
	
	
	

	
	Bath
	1
	x
	2
	8.50
	8.50
	
	144.50
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Walls
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	



	
	Room
	4
	x
	5
	15.50
	
	12.00
	3720.00
	Sft
	
	
	

	
	Verendah
	4
	x
	1
	9.50
	
	12.00
	456.00
	Sft
	
	
	

	
	Bath
	4
	x
	2
	8.50
	
	12.00
	816.00
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	TOTAL
	6466.00
	
	
	
	

	
	Projection
	1
	x
	1
	120.00
	2.50
	
	300.00
	Sft
	
	
	

	
	
	
	
	
	
	Sub Total
	6766.00
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	5
	x
	1
	3.50
	
	6.50
	113.75
	Sft
	
	
	

	
	D2
	1
	x
	1
	2.50
	
	6.50
	16.25
	Sft
	
	
	

	
	W1
	5
	x
	1
	4
	
	5.00
	100.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	230.00
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Net Qty.
	6536.00
	Sft
	8.74
	P.Sft
	

	


7
	Distempering with Berger/ ICI or equivalent synthetic vinyl emulsion paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning in ground floor.
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling and Internal walls Quantity
	1
	x
	2
	6466.0
	
	Net Qty.
	12932.00
	Sft
	26.02
	P.Sft
	

	
8
	Painting old surface in ground floor or basement with
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Qty of Door and Windows
	1
	x
	2
	
	
	Net Qty.
	230.00
	Sft
	35.77
	P.Sft
	

	

9
	1/2 inch ( 13mm) thick cement plaster using Coarse Sand on wall sand columns in basement, plinth and ground floor including making edges, corners and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	6766.0
	
	
	6766.00
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	5
	x
	1
	3.50
	
	6.50
	113.75
	Sft
	
	
	

	
	D2
	1
	x
	1
	2.50
	
	6.50
	16.25
	Sft
	
	
	

	
	W1
	5
	x
	1
	4.00
	
	5.00
	100.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	230.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Net Total
	4536.00
	Sft
	62.45
	
	

	

12
	Providing and laying 1:4:8 hand mixed cement concrete bed under floors using graded shingle or bajri 50 mm and down guage complete with levelling ramming watering and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	1
	15.50
	15.50
	0.25
	60.06
	cft
	
	
	

	
	Verendah
	1
	x
	1
	9.50
	13.50
	0.25
	32.06
	cft
	
	
	

	
	Bath
	1
	x
	2
	8.50
	8.50
	0.25
	36.13
	cft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	128.25
	cft
	332.92
	
	

	






13
	Providing and fixing 1/4" to 3/8" (6mm to 9mm) thick Ceramic Glazed/Matt tiles (Prime Quality) of any colour and size, as directed by Engineer-in-Charge in dado/skirting in ground floor over 1/2" (13mm) thick base of cement mortar 1:3, setting of tiles in slurry of grey cement over mortar base including filling the joints and washing the tiles with white cement slurry of matching color, cleaning & curing.
	
	
	
	
	
	
	
	

	
	Bath
	1
	x
	1
	23.00
	
	7.00
	161.00
	sft
	
	
	

	
	Deduction
	
	
	
	
	
	Total
	161.00
	sft
	
	
	

	
	d1
	1
	x
	1
	2.50
	
	6.50
	16.25
	sft
	
	
	

	
	
	
	
	
	
	
	Total
	16.25
	sft
	
	
	

	
	
	
	
	
	
	
	Net Qty
	144.75
	sft
	213.60
	P.Sft
	

	




14
	Providing and laying 1/4" to 3/8" (6mm to 9mm) thick Glazed/ Matt tiles of any colour and size in ground floor laid over 1" (25mm) thick cement sand mortar base including jointing and washing the tiles with white cement slurry of matching color by using color pigment and curing
	
	
	
	
	
	
	
	



	
	Room
	1
	x
	5
	14.00
	14.00
	
	980.00
	sft
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	12.00
	
	96.00
	sft
	
	
	

	
	Bath
	1
	x
	2
	7.00
	7.00
	
	98.00
	sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	1174.00
	sft
	278.29
	P.Sft
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	ELECTRICAL WORK
	
	
	
	
	
	
	
	
	
	
	

	


30
	Concealed wiring from point to switch with 3/4" (20 mm) dia. PVC conduit length upto 30 ft. (10m) including any switch to switch wiring with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables,
	
	
	
	
	
	
	
	

	
	
	10
	x
	1
	
	
	
	10.00
	Point
	4278.60
	P.Point
	

	


31
	Concealed wiring for 5 Amp. Socket outlets from nearest available circuit with 3/4" (20 mm) dia. PVC conduit length upto 20 ft. (6m) with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables
	
	
	
	
	
	
	
	

	
	
	12
	x
	1
	
	
	
	12.00
	Point
	3358.32
	P.Point
	

	

32
	Supply and install 2-gang, 5 Amp, 250 Volt,. plate type moulded switch including appropriate size plastic box to be fixed recessed in wall.
	
	
	
	
	
	
	
	

	
	
	12
	x
	1
	
	
	
	12.00
	No.
	897.80
	each
	

	

33
	Supply and install combined 2/3 pin 5 Amps, 250 Volt switch socket unit including plastic box to be fixed recessed in wall.
	
	
	
	
	
	
	
	

	
	
	12
	x
	1
	
	
	
	12.00
	No.
	1732.44
	each
	

	
34
	Supply and install Energy Saver electric bulbs
	
	
	
	
	
	
	
	
	
	
	

	
	
	26
	x
	1
	
	
	
	26.00
	No.
	436.00
	P.No
	

	
35
	Supply and install 10" (250 mm) sweep exhaust fan
including plastic louvers.
	
	
	
	
	
	
	
	

	
	
	6
	x
	1
	
	
	
	6.00
	No.
	5564.40
	each
	

	
36
	Installing each number circuit breaker 6 Ampere on same distribution board and bus bar (For outgoing)
	
	
	
	
	
	
	
	

	
	
	1
	x
	2
	
	
	
	2.00
	No.
	3621.00
	P.job
	

	Tuff Tile Work

	
	
	
	
	
	
	
	
	
	
	
	
	

	1.
	Earthwork for embankment lead upto 100 ft. (30m) and compaction by Manual (Maximium Area 250 Sft) labour at optimum moisture
content, dressing to designed section, laying,
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	
	100
	10
	1
	1000
	Cft
	
	
	

	
	
	
	
	
	
	
	
	1000
	Cft
	
	
	

	
	
	
	
	
	
	
	
	
	@
	15.04
	Rs.
	

	2
	Supply and Fixing of Concrete pavers on sand cushion of different designs having thickness of
60 mm, mechnically compressed, minimium strenght of 4500 psi after laboratory testing at factory and random testiing at site as and when desired by the Engineer inchange comple in all respects.  (No  PCC  work  is  premitted
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	
	100
	10
	
	1000
	Sft
	
	
	

	
	
	
	
	
	
	
	
	1000
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	@
	192.06
	Rs.
	

	3
	Providing and laying plain machine mixed cement concrete using coarse sand and crushed aggregate having maximum size upto 11/2" (38mm) & down gauge in foundation including levelling, compacting and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	2
	x
	
	100
	0.5
	0.25
	25
	Cft
	
	
	

	
	
	
	
	
	
	
	
	25
	Cft
	
	
	


	
	
	
	
	
	
	
	
	
	@
	439.27
	Rs.
	

	
	Total Estimated Cost
	

	
	 BRA (Note)      
	

	
	Grand Total Amount (Inclusive of: All Taxes, Labour cost & Transportation charges) 
Note: BRA as per applicable percentage of 2nd schedule of Repair & Maintenance on payments other than Balochistan consolidated fund. 
	







	[bookmark: BHU_Peer_koh]DETAILED ESTIMATE FOR REHABILITATION BASIC HEALTH UNIT PEER KOH DISTRICT DERA BUGTI

	

	S.
No.
	Description of work
	No.
	Measurement
	Quantity
	Unit
	Rate
	Amount

	
	
	
	Length
	Width
	Height
	
	
	
	

	
1
	Dismantling reinforced cement concrete, separating reinforcement from concrete,
clearing and straightening the same
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	4
	14.00
	14.00
	0.50
	392.00
	cft
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	10.00
	0.50
	40.00
	cft
	
	
	

	
	
	
	
	
	
	
	
	432.00
	cft
	
	
	

	
2
	Providing rolled steel joists and channels including hoisting and fixing in position in cement concrete but excluding the cost of
cement concrete
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	4
	14.00
	14
	
	784.00
	kgs
	
	
	

	
	
	
	
	
	
	
	
	784.00
	
	
	
	

	3
	Providing M.S. Tees, angles and flats
including fixing in position.
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	4
	14.00
	14.00
	1.50
	1176.00
	lbs
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	10.00
	1.50
	120.00
	lbs
	
	
	

	
	
	
	
	
	
	
	
	1296.00
	lbs
	
	
	

	
	
	
	
	5406/2.204
	
	
	588.02
	kg
	
	
	

	




4
	Providing and laying second class brick tile roofing comprising 4 inches (100mm) thick earth and 1 inch (25 mm) thick mud plaster with gobri leeping over 1/2 inch (13mm) thick cement plaster 1:6 with 34 lbs./100 Sq.ft.(1.65 Kg./Sq.m.) hot bitumen coating sand blended in one coat, provided over one layer of tiles 12" x 6"x 2" laid in 1:6 cement sand mortar including 1:2 cement sand pointing underside of tiles including curing
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	4
	14.00
	14.00
	
	784.00
	Sft
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	10.00
	
	80.00
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	864.00
	Sft
	
	
	

	5
	Providing and laying 1:2:4 P.C.C roof screeding using crushed stone 3/4" (19mm) including formwork, consolidation, finishing and curing. 1-1/2" (37.5mm) nominal thick P.C.C. roof screeding
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	4
	14.00
	14.00
	
	784.00
	Sft
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	10.00
	
	80.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	864.00
	Sft
	
	
	

	6
	Scraping, rubbing and cleaning of oil bound distemper from ceiling and walls including removal of rubbish in ground floor
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	4
	14.00
	14.00
	
	784.00
	Sft
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	10.00
	
	80.00
	Sft
	
	
	

	
	Walls
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	2
	x
	4
	28.00
	
	12.00
	2688.00
	Sft
	
	
	

	
	
	2
	x
	1
	18.00
	
	12.00
	432.00
	Sft
	
	
	

	
	
	
	
	
	
	
	TOTAL
	3984.00
	
	
	
	

	
	Projection
	1
	x
	1
	120.00
	2.50
	
	300.00
	Sft
	
	
	

	
	
	
	
	
	
	Sub Total
	4284.00
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	4
	x
	1
	3.50
	
	6.50
	91.00
	Sft
	
	
	

	
	D2
	2
	x
	1
	2.50
	
	6.50
	32.50
	Sft
	
	
	

	
	W1
	4
	x
	1
	4
	
	5.00
	80.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	203.50
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Net Qty.
	4080.50
	Sft
	
	
	

	7
	Distempering with Berger/ ICI or equivalent synthetic vinyl emulsion paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning in ground floor.
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling and Internal walls Quantity
	1
	x
	2
	7344.0
	
	Net Qty.
	14688.00
	Sft
	
	
	

	8
	Painting old surface in ground floor or basement with
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Qty of Door and Windows
	1
	x
	2
	
	
	Net Qty.
	203.50
	Sft
	
	
	

	9
	1/2 inch ( 13mm) thick cement plaster using Coarse Sand on wall sand columns in basement, plinth and ground floor including making edges, corners and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	4284.0
	
	
	4284.00
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	4
	x
	1
	3.50
	
	6.50
	91.00
	Sft
	
	
	

	
	D2
	2
	x
	1
	2.50
	
	6.50
	32.50
	Sft
	
	
	

	
	W1
	4
	x
	1
	4.00
	
	5.00
	80.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	203.50
	Sft
	
	
	

	
	
	
	
	
	
	Net Total
	4080.50
	Sft
	
	
	

	10
	Providing and laying 1:4:8 hand mixed cement concrete bed under floors using graded shingle or bajri 50 mm and down guage complete with levelling ramming
watering and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	4
	14.00
	14.00
	0.25
	196.00
	cft
	
	
	

	
	
	1
	x
	1
	8.00
	10.00
	0.25
	20.00
	cft
	
	
	

	
	
	
	
	
	
	
	
	324.00
	cft
	
	
	

	11
	Providing and fixing 1/4" to 3/8" (6mm to 9mm) thick Ceramic Glazed/Matt tiles (Prime Quality) of any colour and size, as directed by Engineer-in-Charge in dado/skirting in ground floor over 1/2" (13mm) thick base of cement mortar 1:3, setting of tiles in slurry of grey cement over mortar base including filling the joints and washing the tiles with white cement slurry of matching color, cleaning & curing.
	
	
	
	
	
	
	
	

	
	Room
	4
	x
	1
	14.00
	
	14.00
	784.00
	sft
	
	
	

	
	Verrendah
	2
	x
	1
	10.00
	
	8.00
	160.00
	sft
	
	
	

	
	Deduction
	
	
	
	
	
	Total
	1227.20
	sft
	
	
	

	
	d1
	2
	x
	1
	2.50
	
	6.50
	32.50
	sft
	
	
	

	
	
	
	
	
	
	
	Total
	32.50
	sft
	
	
	

	
	
	
	
	
	
	
	Net Qty
	1194.70
	sft
	
	
	

	12
	Providing and laying 1/4" to 3/8" (6mm to 9mm) thick Glazed/ Matt tiles of any colour and size in ground floor laid over 1" (25mm) thick cement sand mortar base including jointing and washing the tiles with white cement slurry of matching color by using color pigment and curing
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	4
	14.00
	14.00
	
	1064.00
	cft
	
	
	

	
	Verrendah
	1
	x
	1
	8.00
	10.00
	
	80.00
	cft
	
	
	

	
	
	
	
	
	
	
	
	1144.00
	sft
	
	
	

	13
	Providing and fixing steel grated single leaf door with1/16"(1.6mm) thick M.S. sheeting and locking arrangement,angleiron2"x2"x3/8"frame middle strip,1/4"thick gusset plate3"x3" ateached geand3/4"M.S squar eorround barsat4"c/c includingtwocoatsof red oxide paint.
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Main Door
	1
	x
	1
	5
	
	7
	35.00
	
	
	
	

	
	D
	4
	x
	1
	3.50
	
	6.50
	91.00
	Sft
	
	
	

	
	D2
	2
	x
	1
	2.50
	
	6.50
	32.50
	Sft
	
	
	

	
	ELECTRICAL WORK
	
	
	
	
	
	
	
	
	
	
	

	15
	Concealed wiring from point to switch with 3/4" (20 mm) dia. PVC conduit length upto 30 ft. (10m) including any switch to switch wiring with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables,
	
	
	
	
	
	
	
	

	
	
	20
	x
	1
	
	
	
	20.00
	Point
	
	
	

	16
	Concealed wiring for 5 Amp. Socket outlets from nearest available circuit with 3/4" (20 mm) dia. PVC conduit length upto 20 ft. (6m) with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables
	
	
	
	
	
	
	
	

	
	
	20
	x
	1
	
	
	
	20.00
	Point
	
	
	

	17
	Supply and install 2-gang, 5 Amp, 250 Volt,. plate type moulded switch including appropriate size plastic box to be fixed recessed in wall.
	
	
	
	
	
	
	
	

	
	
	5
	x
	1
	
	
	
	5.00
	No.
	
	
	

	18
	Supply and install combined 2/3 pin 5 Amps, 250 Volt switch socket unit including plastic box to be fixed recessed in wall.
	
	
	
	
	
	
	
	

	
	
	5
	x
	1
	
	
	
	5.00
	No.
	
	
	

	19
	Supply and install Energy Saver electric bulbs
	
	
	
	
	
	
	
	
	
	
	

	
	
	5
	x
	1
	
	
	
	5.00
	No.
	
	
	

	20
	Supply and install 10" (250 mm) sweep exhaust fan
including plastic louvers.
	
	
	
	
	
	
	
	

	
	
	5
	x
	1
	
	
	
	5.00
	No.
	
	
	

	21
	Installing each number circuit breaker 6 Ampere on same distribution board and bus bar (For outgoing)
	
	
	
	
	
	
	
	

	
	
	5
	x
	2
	
	
	
	10.00
	No.
	
	
	

	
	Total Estimated Cost
	

	
	 BRA (Note)      
	

	
	Grand Total Amount (Inclusive of: All Taxes, Labour cost & Transportation charges) 
Note: BRA as per applicable percentage of 2nd schedule of Repair & Maintenance on payments other than Balochistan consolidated fund. 
	



	[bookmark: BHU_Peetokh]DETAILED ESTIMATE FOR REHABILITATION BASIC HEALTH UNIT PEETOKH DISTRICT DERA BUGTI

	

	S.
No.
	Description of work
	No.
	Measurement
	Quantity
	Unit
	Rate
	Amount

	
	
	
	Length
	Width
	Height
	
	
	
	

	5
	Providing and laying 1:2:4 P.C.C roof screeding using crushed stone 3/4" (19mm) including formwork, consolidation, finishing and curing. 1-1/2" (37.5mm) nominal thick P.C.C. roof screeding
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	15.00
	14.00
	
	1050.00
	Sft
	
	
	

	
	Verendah
	1
	x
	1
	6.00
	12.00
	
	72.00
	Sft
	
	
	

	
	Bath
	1
	x
	1
	7.00
	7.00
	
	49.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	1346.40
	Sft
	
	
	

	9
	1/2 inch ( 13mm) thick cement plaster using Coarse Sand on wall sand columns in basement, plinth and ground floor including making edges, corners and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	15.00
	14.00
	
	1050.00
	Sft
	
	
	

	
	Verendah
	1
	x
	1
	6.00
	12.00
	
	72.00
	Sft
	
	
	

	
	Bath
	1
	x
	1
	7.00
	7.00
	
	49.00
	Sft
	
	
	

	
	Walls
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	4
	x
	5
	15.00
	11.00
	
	3300.00
	Sft
	
	
	

	
	Verendah
	4
	x
	1
	6.00
	10.00
	
	240.00
	Sft
	
	
	

	
	Bath
	4
	x
	1
	7.00
	11.00
	
	308.00
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	Net Total
	6524.70
	Sft
	
	
	

	6
	Scraping, rubbing and cleaning of oil bound distemper from ceiling and walls including removal of rubbish in ground floor
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling
	
	
	
	
	
	
	
	
	
	
	

	
	Verendah
	1
	x
	1
	6524.70
	1.00
	
	6524.70
	Sft
	
	
	

	
	
	
	
	
	
	Sub Total
	6524.70
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	4
	x
	1
	3.50
	
	6.50
	91.00
	Sft
	
	
	

	
	D2
	2
	x
	1
	2.50
	
	6.50
	32.50
	Sft
	
	
	

	
	W1
	4
	x
	1
	4
	
	5.00
	80.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	203.50
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Net Qty.
	6321.20
	Sft
	
	
	

	7
	Distempering with Berger/ ICI or equivalent synthetic vinyl emulsion paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning in ground floor.
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling and Internal walls Quantity
	1
	x
	2
	8217.6
	
	Net Qty.
	16435.12
	Sft
	
	
	

	8
	Painting old surface in ground floor or basement with
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Qty of Door and Windows
	1
	x
	2
	
	
	Net Qty.
	203.50
	Sft
	
	
	

	10
	Providing and laying 1:4:8 hand mixed cement concrete bed under floors using graded shingle or bajri 50 mm and down guage complete with levelling ramming watering and
curing.
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	5
	15.00
	15.00
	0.25
	281.25
	cft
	
	
	

	
	
	1
	x
	1
	6.00
	10.00
	0.25
	15.00
	cft
	
	
	

	
	
	
	
	
	
	
	
	444.38
	cft
	
	
	

	Tuff Tile Work

	
	
	
	
	
	
	
	
	
	
	
	
	

	1.
	Earthwork for embankment lead upto 100 ft. (30m) and compaction by Manual (Maximium Area 250 Sft) labour at optimum moisture
content, dressing to designed section, laying,
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	
	120
	10
	1
	1200
	Cft
	
	
	

	
	
	
	
	
	
	
	
	1200
	Cft
	
	
	

	
	
	
	
	
	
	
	
	
	@
	
	
	

	2
	Supply and Fixing of Concrete pavers on sand cushion of different designs having thickness of 60 mm, mechnically compressed, minimium strenght of 4500 psi after laboratory testing at factory and random testiing at site as and when desired by the Engineer inchange
comple in all respects. (No PCC work is
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	
	140
	10
	
	1400
	Sft
	
	
	

	
	
	
	
	
	
	
	
	1400
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	@
	
	
	

	3
	Providing and laying plain machine mixed cement concrete using coarse sand and crushed aggregate having maximum size upto 11/2" (38mm) & down gauge in foundation
including levelling, compacting and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	2
	x
	
	140
	0.5
	0.25
	35
	Cft
	
	
	

	
	
	
	
	
	
	
	
	35
	Cft
	
	
	

	
	
	
	
	
	
	
	
	
	@
	
	
	

	
	Total Estimated Cost
	

	
	 BRA (Note)      
	

	
	Grand Total Amount (Inclusive of: All Taxes, Labour cost & Transportation charges) 
Note: BRA as per applicable percentage of 2nd schedule of Repair & Maintenance on payments other than Balochistan consolidated fund. 
	



	DETAILED ESTIMATE FOR REHABILITATION BASIC HEALTH UNIT SERLOPE DISTRICT DERA BUGTI

	

	S.
No.
	Description of work
	No.
	Measurement
	Quantity
	Unit
	Rate
	Amount

	
	
	
	Length
	Width
	Height
	
	
	
	

	
1
	Dismantling reinforced cement concrete,
separating reinforcement from concrete, clearing and straightening the same
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	14.00
	14.00
	0.50
	490.00
	cft
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	12.00
	0.50
	48.00
	cft
	
	
	

	
	Bath
	1
	x
	1
	7.00
	7.00
	0.50
	24.50
	cft
	
	
	

	
	
	
	
	
	
	
	
	562.50
	cft
	207.62
	
	

	
2
	Providing rolled steel joists and channels including hoisting and fixing in position in cement concrete but excluding the cost of
cement concrete
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	14.00
	4
	
	280.00
	kgs
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	4
	
	32.00
	kgs
	
	
	

	
	Bath
	1
	x
	1
	7.00
	4
	
	28.00
	kgs
	
	
	

	
	
	
	
	
	
	
	
	340.00
	
	394.18
	
	

	3
	Providing M.S. Tees, angles and flats including
fixing in position.
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	14.00
	14.00
	1.50
	1470.00
	lbs
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	12.00
	1.50
	144.00
	lbs
	
	
	

	
	Bath
	1
	x
	1
	7.00
	7.00
	1.50
	73.50
	lbs
	
	
	

	
	
	
	
	
	
	
	
	1687.50
	lbs
	
	
	

	
	
	
	
	5406/2.204
	
	
	765.65
	kg
	406.97
	
	

	




4
	Providing and laying second class brick tile roofing comprising 4 inches (100mm) thick earth and 1 inch (25 mm) thick mud plaster with gobri leeping over 1/2 inch (13mm) thick cement plaster 1:6 with 34 lbs./100 Sq.ft.(1.65 Kg./Sq.m.) hot bitumen coating sand blended in one coat, provided over one layer of tiles 12" x 6"x 2" laid in 1:6 cement sand mortar including 1:2 cement sand pointing underside of tiles including curing
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	14.00
	14.00
	
	980.00
	Sft
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	12.00
	
	96.00
	Sft
	
	
	

	
	Bath
	1
	x
	1
	7.00
	7.00
	
	49.00
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	1125.00
	Sft
	204.82
	
	

	5
	Providing and laying 1:2:4 P.C.C roof screeding using crushed stone 3/4" (19mm) including formwork, consolidation, finishing and curing. 1-1/2" (37.5mm) nominal thick P.C.C. roof screeding
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	15.50
	15.50
	
	1201.25
	Sft
	
	
	

	
	Verendah
	1
	x
	1
	9.50
	13.50
	
	128.25
	Sft
	
	
	

	
	Bath
	1
	x
	1
	8.50
	8.50
	
	72.25
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Total
	1401.75
	Sft
	121.40
	P.Sft
	

	6
	Scraping, rubbing and cleaning of oil bound distemper from ceiling and walls including removal of rubbish in ground floor
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	15.50
	15.50
	
	1201.25
	Sft
	
	
	

	
	Verendah
	1
	x
	1
	9.50
	13.50
	
	128.25
	Sft
	
	
	

	
	Bath
	1
	x
	1
	8.50
	8.50
	
	72.25
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Walls
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	4
	x
	5
	15.50
	
	12.00
	3720.00
	Sft
	
	
	

	
	Verendah
	4
	x
	1
	9.50
	
	12.00
	456.00
	Sft
	
	
	

	
	Bath
	4
	x
	1
	8.50
	
	12.00
	408.00
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	TOTAL
	5985.75
	
	
	
	

	
	Projection
	1
	x
	1
	120.00
	2.50
	
	300.00
	Sft
	
	
	

	
	
	
	
	
	
	Sub Total
	6285.75
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	5
	x
	1
	3.50
	
	6.50
	113.75
	Sft
	
	
	

	
	D2
	1
	x
	1
	2.50
	
	6.50
	16.25
	Sft
	
	
	

	
	W1
	5
	x
	1
	4
	
	5.00
	100.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	230.00
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Net Qty.
	6055.75
	Sft
	8.74
	P.Sft
	

	7
	Distempering with Berger/ ICI or equivalent synthetic vinyl emulsion paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning in ground floor.
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling and Internal walls Quantity
	1
	x
	2
	5985.8
	
	Net Qty.
	11971.50
	Sft
	26.02
	P.Sft
	

	8
	Painting old surface in ground floor or basement with
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Qty of Door and Windows
	1
	x
	2
	
	
	Net Qty.
	230.00
	Sft
	35.77
	P.Sft
	

	9
	1/2 inch ( 13mm) thick cement plaster using Coarse Sand on wall sand columns in basement, plinth and ground floor including making edges, corners and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	6285.8
	
	
	6285.75
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	5
	x
	1
	3.50
	
	6.50
	113.75
	Sft
	
	
	

	
	D2
	1
	x
	1
	2.50
	
	6.50
	16.25
	Sft
	
	
	

	
	W1
	5
	x
	1
	4.00
	
	5.00
	100.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	230.00
	Sft
	
	
	

	
	
	
	
	
	
	Net Total
	4055.75
	Sft
	62.45
	
	

	12
	Providing and laying 1:4:8 hand mixed cement concrete bed under floors using graded shingle or bajri 50 mm and down guage complete with levelling ramming watering and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	1
	15.50
	15.50
	0.25
	60.06
	cft
	
	
	

	
	Verendah
	1
	x
	1
	9.50
	13.50
	0.25
	32.06
	cft
	
	
	

	
	Bath
	1
	x
	1
	8.50
	8.50
	0.25
	18.06
	cft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	110.19
	cft
	332.92
	
	

	13
	Providing and fixing 1/4" to 3/8" (6mm to 9mm) thick Ceramic Glazed/Matt tiles (Prime Quality) of any colour and size, as directed by Engineer-in-Charge in dado/skirting in ground floor over 1/2" (13mm) thick base of cement mortar 1:3, setting of tiles in slurry of grey cement over mortar base including filling the joints and washing the tiles with white cement slurry of matching color, cleaning & curing.
	
	
	
	
	
	
	
	

	
	Bath
	1
	x
	1
	23.00
	
	7.00
	161.00
	sft
	
	
	

	
	Deduction
	
	
	
	
	
	Total
	161.00
	sft
	
	
	

	
	d1
	1
	x
	1
	2.50
	
	6.50
	16.25
	sft
	
	
	

	
	
	
	
	
	
	
	Total
	16.25
	sft
	
	
	

	
	
	
	
	
	
	
	Net Qty
	144.75
	sft
	213.60
	P.Sft
	

	14
	Providing and laying 1/4" to 3/8" (6mm to 9mm) thick Glazed/ Matt tiles of any colour and size in ground floor laid over 1" (25mm) thick cement sand mortar base including jointing and washing the tiles with white cement slurry of matching color by using color pigment and curing
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	5
	14.00
	14.00
	
	980.00
	sft
	
	
	

	
	Verendah
	1
	x
	1
	8.00
	12.00
	
	96.00
	sft
	
	
	

	
	Bath
	1
	x
	1
	7.00
	7.00
	
	49.00
	sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	1125.00
	sft
	278.29
	P.Sft
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	ELECTRICAL WORK
	
	
	
	
	
	
	
	
	
	
	

	30
	Concealed wiring from point to switch with 3/4" (20 mm) dia. PVC conduit length upto 30 ft. (10m) including any switch to switch wiring with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables,
	
	
	
	
	
	
	
	

	
	
	10
	x
	1
	
	
	
	10.00
	Point
	4278.60
	P.Poi
	

	31
	Concealed wiring for 5 Amp. Socket outlets from nearest available circuit with 3/4" (20 mm) dia. PVC conduit length upto 20 ft. (6m) with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables
	
	
	
	
	
	
	
	

	
	
	12
	x
	1
	
	
	
	12.00
	Point
	3358.32
	P.Poi
	

	32
	Supply and install 2-gang, 5 Amp, 250 Volt,. plate type moulded switch including appropriate size plastic box to be fixed recessed in wall.
	
	
	
	
	
	
	
	

	
	
	12
	x
	1
	
	
	
	12.00
	No.
	897.80
	each
	

	33
	Supply and install combined 2/3 pin 5 Amps, 250 Volt switch socket unit including plastic box to be fixed recessed in wall.
	
	
	
	
	
	
	
	

	
	
	12
	x
	1
	
	
	
	12.00
	No.
	1732.44
	each
	

	34
	Supply and install Energy Saver electric bulbs
	
	
	
	
	
	
	
	
	
	
	

	
	
	26
	x
	1
	
	
	
	26.00
	No.
	436.00
	P.No
	

	35
	Supply and install 10" (250 mm) sweep exhaust fan
including plastic louvers.
	
	
	
	
	
	
	
	

	
	
	6
	x
	1
	
	
	
	6.00
	No.
	5564.40
	each
	

	36
	Installing each number circuit breaker 6 Ampere on same distribution board and bus bar (For outgoing)
	
	
	
	
	
	
	
	

	
	
	1
	x
	2
	
	
	
	2.00
	No.
	3621.00
	P.job
	

	Tuff Tile Work

	
	
	
	
	
	
	
	
	
	
	
	
	

	1.
	Earthwork for embankment lead upto 100 ft. (30m) and compaction by Manual (Maximium Area 250 Sft) labour at optimum moisture content, dressing to designed section, laying,
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	
	100
	10
	1
	1000
	Cft
	
	
	

	
	
	
	
	
	
	
	
	1000
	Cft
	
	
	

	
	
	
	
	
	
	
	
	
	Rs.
	15.04
	Rs.
	

	2
	Supply and Fixing of Concrete pavers on sand cushion of different designs having thickness of
60 mm, mechnically compressed, minimium strenght of 4500 psi after laboratory testing at factory and random testiing at site as and when desired by the Engineer inchange comple in all respects. (No PCC work is premitted underneath
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	
	100
	10
	
	1000
	Sft
	
	
	

	
	
	
	
	
	
	
	
	1000
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	@
	192.06
	Rs.
	

	3
	Providing and laying plain machine mixed cement concrete using coarse sand and crushed aggregate having maximum size upto 11/2" (38mm) & down gauge in foundation including levelling, compacting and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	2
	x
	
	100
	0.5
	0.25
	25
	Cft
	
	
	

	
	
	
	
	
	
	
	
	25
	Cft
	
	
	

	
	
	
	
	
	
	
	
	
	Rs.
	439.27
	Rs.
	

	
	
Total Estimated Cost
	

	
	 BRA (Note)      
	

	
	Grand Total Amount (Inclusive of: All Taxes, Labour cost & Transportation charges) 

Note: BRA as per applicable percentage of 2nd schedule of Repair & Maintenance on payments other than Balochistan consolidated fund. 
	


































	[bookmark: DO_Dera_Bugti_(Additional_work)]DETAILED ESTIMATE FOR CONSTRUCTION WORK AT DISTRICT OFFICE PPHI DISTRICT DERA BUGTI

	

	S.
No.
	Description of work
	No.
	Measurement
	Quantity
	Unit
	Rate
	Amount

	
	
	
	Length
	Width
	Height
	
	
	
	

	1
	Excavation in foundation of buildings including layout, dressing, refilling around structures with excavated earth, watering & ramming lead upto 100 ft. (30m) & lift upto 5 ft.
	
	
	
	
	
	
	
	

	
	Multi Purpose Hall
	1
	x
	4
	20.00
	2.00
	2.50
	400.00
	cft
	
	
	

	
	Additional Room
	1
	x
	4
	14.00
	2.00
	2.50
	280.00
	cft
	
	
	

	
	Common Baths
	1
	x
	4
	8.00
	2.00
	2.50
	160.00
	cft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	2
	Providing and laying cement concrete using approved coarse sand andcrushed aggregate 3/4" (19mm) & down gauge in foundation includingleveling, compacting and curing..
	
	
	
	
	
	
	
	

	
	Multi Purpose Hall
	1
	x
	4
	20.00
	2.00
	2.50
	400.00
	cft
	
	
	

	
	Additional Room
	1
	x
	4
	14.00
	2.00
	2.50
	280.00
	cft
	
	
	

	
	Common Baths
	1
	x
	4
	8.00
	2.00
	2.50
	160.00
	cft
	
	
	

	3
	Providing,  fabricating  and  laying  deformed  Grade
40 steel reinforcement (deformed bar) for all kinds of R.C.C work in foundation, plinth and ground floor including the cost of straightening, removal of rust, cutting, bending, binding, wastage and providing such over-laps as are not shown on the drawings.
	
	
	
	
	
	
	
	

	
	Qty of Plinth Bend 4 #4
	4
	x
	1
	236.25
	
	0.667
	630.32
	lbs
	
	
	

	
	Rings #3 at 9"' c/c
	315
	x
	1
	4.50
	
	0.375
	531.56
	lbs
	
	
	

	
	
	
	
	
	
	
	Total
	1161.88
	lbs
	
	
	

	
	
	
	
	
	
	
	Total
	0.5187
	Ton
	
	
	

	5
	Providing and laying first class solid burnt brick masonry (Brick Strength:1800psi-2000psi) including scaffolding, raking out joints and curing in substructure i/c cost of testing
	
	
	
	
	
	
	
	

	
	Multi Purpose Hall
	
	
	
	
	
	
	
	
	
	
	

	
	1st step
	1
	x
	4
	20.000
	1.87
	0.75
	112.20
	cft
	
	
	

	
	2nd step
	1
	x
	4
	20.000
	1.5
	1.00
	120.00
	cft
	
	
	

	
	3rd step
	1
	x
	4
	20.000
	1.125
	1.25
	112.50
	cft
	
	
	

	
	Additional Room
	
	
	
	
	
	
	
	
	
	
	

	
	1st step
	1
	x
	4
	14.000
	1.87
	0.75
	78.54
	cft
	
	
	

	
	2nd step
	1
	x
	4
	14.000
	1.5
	1.00
	84.00
	cft
	
	
	

	
	3rd step
	1
	x
	4
	14.000
	1.125
	1.25
	78.75
	cft
	
	
	

	
	Common Baths
	
	
	
	
	
	
	
	
	
	
	

	
	1st step
	1
	x
	4
	8.000
	1.87
	0.75
	44.88
	cft
	
	
	

	
	2nd step
	1
	x
	4
	8.000
	1.5
	1.00
	48.00
	cft
	
	
	

	
	3rd step
	1
	x
	4
	8.000
	1.125
	1.25
	45.00
	cft
	
	
	

	
	
	
	
	
	
	
	Total
	723.87
	cft
	
	
	

	6
	Providing and laying 1:2:4 cement concrete using approved coarse sand and crushed aggregate 3/4" (19mm.) and down gauge in plinth band of required shape or section including formwork and its removal, compacting and curing in ground floor but excluding the cost of reinforcement.
	
	
	
	
	
	
	
	

	
	Plinth bend
	
	
	
	
	
	
	
	
	
	
	

	
	Multi Purpose Hall
	1
	x
	4
	20.00
	1.125
	1.25
	112.50
	cft
	
	
	

	
	Additional Room
	1
	x
	4
	14.00
	1.125
	1.25
	78.75
	cft
	
	
	

	
	Common Baths
	1
	x
	4
	8.00
	1.125
	1.25
	45.00
	cft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	7
	Providing and laying first class solid burnt brick masonry (Brick Strength: 1800psi - 2000psi) including scaffolding, raking out joints and curing in ground floor superstructure and i/c cost of testing. Above 4.5" (115mm) nominal thick
	
	
	
	
	
	
	
	

	
	Brick Masonary
	
	
	
	
	
	
	
	
	
	
	

	
	Multi Purpose Hall
	1
	x
	4
	20.00
	0.75
	11.00
	660.00
	cft
	
	
	

	
	Additional Room
	1
	x
	4
	14.00
	0.75
	11.00
	462.00
	cft
	
	
	

	
	Common Baths
	1
	x
	4
	8.00
	0.75
	11.00
	264.00
	cft
	
	
	

	9
	3/4 inch (19mm) thick cement plaster 1:4 using Coarse Sand on walls and columns in ground floor including making edges, corners and curing.
	
	
	
	
	
	
	
	

	
	Ceiling
	
	
	
	
	
	
	
	
	
	
	

	
	Multi Purpose Hall
	1
	x
	1
	20.00
	20.00
	
	400.00
	Sft
	
	
	



	
	Additional Room
	1
	x
	1
	14.00
	14.00
	
	196.00
	Sft
	
	
	

	
	Common Baths
	1
	x
	1
	8.00
	8.00
	
	64.00
	Sft
	
	
	

	
	Walls
	
	
	
	
	
	
	
	
	
	
	

	
	Multi Purpose Hall
	1
	x
	4
	20.00
	
	11.00
	880.00
	Sft
	
	
	

	
	Additional Room
	1
	x
	4
	14.00
	
	11.00
	616.00
	Sft
	
	
	

	
	Common Baths
	1
	x
	4
	8.00
	
	11.00
	352.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	2508.00
	Sft
	
	
	

	
2
	Providing rolled steel joists and channels including hoisting and fixing in position in cement concrete but excluding the cost of
cement concrete
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Multi Purpose Hall
	1
	x
	1
	20.00
	4
	
	80.00
	kgs
	
	
	

	
	Additional Room
	1
	x
	1
	14.00
	4
	
	56.00
	kgs
	
	
	

	
	Common Baths
	1
	x
	1
	8.00
	4
	
	32.00
	kgs
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	168.00
	
	
	
	

	3
	Providing M.S. Tees, angles and flats including
fixing in position.
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Multi Purpose Hall
	1
	x
	1
	20.00
	14.00
	1.50
	420.00
	lbs
	
	
	

	
	Additional Room
	1
	x
	1
	14.00
	10.00
	1.50
	210.00
	lbs
	
	
	

	
	Common Baths
	1
	x
	1
	8.00
	10.00
	1.50
	120.00
	lbs
	
	
	

	
	
	
	
	
	
	
	
	750.00
	lbs
	
	
	

	
	
	
	
	5406/2.204
	
	
	340.29
	kg
	
	
	

	




4
	Providing and laying second class brick tile roofing comprising 4 inches (100mm) thick earth and 1 inch (25 mm) thick mud plaster with gobri leeping over 1/2 inch (13mm) thick cement plaster 1:6 with 34 lbs./100 Sq.ft.(1.65 Kg./Sq.m.) hot bitumen coating sand blended in one coat, provided over one layer of tiles 12" x 6"x 2" laid in 1:6 cement sand mortar including 1:2 cement sand pointing underside of tiles including curing
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Multi Purpose Hall
	1
	x
	1
	20.00
	20.00
	
	400.00
	Sft
	
	
	

	
	Additional Room
	1
	x
	1
	14.00
	14.00
	
	196.00
	Sft
	
	
	

	
	Common Baths
	1
	x
	1
	8.00
	8.00
	
	64.00
	Sft
	
	
	

	
	
	
	
	
	
	
	
	660.00
	Sft
	
	
	

	5
	Providing and laying 1:2:4 P.C.C roof screeding using crushed stone 3/4" (19mm) including formwork, consolidation, finishing and curing. 1-1/2" (37.5mm) nominal thick P.C.C. roof screeding
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Multi Purpose Hall
	1
	x
	4
	20.00
	20.00
	0.25
	400.00
	cft
	
	
	

	
	Additional Room
	1
	x
	4
	14.00
	14.00
	0.25
	196.00
	cft
	
	
	

	
	Common Baths
	1
	x
	4
	8.00
	8.00
	0.25
	64.00
	cft
	
	
	

	
	
	
	
	
	
	
	Total
	660.00
	Sft
	
	
	

	6
	Scraping, rubbing and cleaning of oil bound distemper from ceiling and walls including removal of rubbish in ground floor
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	2508.00
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Net Qty.
	2508.00
	Sft
	
	
	

	7
	Distempering with Berger/ ICI or equivalent synthetic vinyl emulsion paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning in ground floor.
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling and Internal walls Quantity
	1
	x
	2
	2508.0
	
	Net Qty.
	5016.00
	Sft
	
	
	

	9
	1/2 inch ( 13mm) thick cement plaster using Coarse Sand on wall sand columns in basement, plinth and ground floor including making edges, corners and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	2508.0
	
	
	2508.00
	Sft
	
	
	

	
	
	
	
	
	
	Net Total
	2508.00
	Sft
	
	
	

	10
	Providing and laying 1:4:8 hand mixed cement concrete bed under floors using graded shingle or bajri 50 mm and down guage complete with levelling ramming watering and
curing.
	
	
	
	
	
	
	
	
	
	
	

	
	Multi Purpose Hall
	1
	x
	1
	20.00
	20.00
	0.33
	133.20
	cft
	
	
	

	
	Additional Room
	1
	x
	1
	14.00
	14.00
	0.33
	65.27
	cft
	
	
	

	
	Common Baths
	1
	x
	1
	8.00
	8.00
	0.33
	21.31
	cft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	329.67
	cft
	
	
	

	12
	Providing and laying 1/4" to 3/8" (6mm to 9mm) thick Glazed/ Matt tiles of any colour and size in ground floor laid over 1" (25mm) thick cement sand mortar base including jointing and washing the tiles with white cement slurry of matching color by using color pigment and curing
	
	
	
	
	
	
	
	

	
	Multi Purpose Hall
	1
	x
	1
	20.00
	20.00
	
	400.00
	Sft
	
	
	

	
	Additional Room
	1
	x
	1
	14.00
	14.00
	
	196.00
	Sft
	
	
	

	
	Common Baths
	1
	x
	1
	8.00
	8.00
	
	64.00
	Sft
	
	
	

	
	
	
	
	
	
	
	
	660.00
	sft
	
	
	

	
	ELECTRICAL WORK
	
	
	
	
	
	
	
	
	
	
	

	15
	Concealed wiring from point to switch with 3/4" (20 mm) dia. PVC conduit length upto 30 ft. (10m) including any switch to switch wiring with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables,
	
	
	
	
	
	
	
	

	
	
	20
	x
	1
	
	
	
	20.00
	Point
	
	
	

	16
	Concealed wiring for 5 Amp. Socket outlets from nearest available circuit with 3/4" (20 mm) dia. PVC conduit length upto 20 ft. (6m) with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables
	
	
	
	
	
	
	
	

	
	
	20
	x
	1
	
	
	
	20.00
	Point
	
	
	

	17
	Supply and install 2-gang, 5 Amp, 250 Volt,. plate type moulded switch including appropriate size plastic box to be fixed recessed in wall.
	
	
	
	
	
	
	
	

	
	
	5
	x
	1
	
	
	
	5.00
	No.
	
	
	

	18
	Supply and install combined 2/3 pin 5 Amps, 250 Volt switch socket unit including plastic box to be fixed recessed in wall.
	
	
	
	
	
	
	
	

	
	
	5
	x
	1
	
	
	
	5.00
	No.
	
	
	

	19
	Supply and install Energy Saver electric bulbs
	
	
	
	
	
	
	
	
	
	
	

	
	
	5
	x
	1
	
	
	
	5.00
	No.
	
	
	

	20
	Supply and install 10" (250 mm) sweep exhaust fan
including plastic louvers.
	
	
	
	
	
	
	
	

	
	
	5
	x
	1
	
	
	
	5.00
	No.
	
	
	

	21
	Installing each number circuit breaker 6 Ampere on same distribution board and bus bar (For outgoing)
	
	
	
	
	
	
	
	

	
	
	5
	x
	2
	
	
	
	10.00
	No.
	
	
	

	
	Plumbing
	
	
	
	
	
	
	
	
	
	
	



	17
	Providing and fixing squatting type water closet with integral treads ICL Boch/Karam Cera or approved equivalent make including cost of inlet pipe cistern and lid cistern kit, stop cock deluxe type and other accessories, fittings, brackets, PVC down pipe, rubber rings/washers.
	
	
	
	
	
	
	
	

	
	
	
1
	
x
	
2
	
	
	
	
2.00
	
No
	
	
	

	18
	Providing and fixing export quality glazed earthen ware wash basin manufactured by ICL Boch/Karam Cera or equivalent approved make with single hole chromium plated mixer tap 1/2" (15mm), pillar tap delux, stop cocks,
	
	
	
	
	
	
	
	

	
	
	1
	x
	2
	
	
	
	2.00
	No
	
	
	

	19
	Providing, laying, cutting, jointing, testing and disinfecting PVC pipes confirming to BSS-3505/PS-3051 complete in all respects.
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	
	
	
	300.00
	Rft
	
	
	

	20
	Providing, laying, cutting, jointing, testing and disinfecting PPRC pipes (25mm) confirming to ISO 4427, PN-20, complete in all respects with specials and valves etc. including all fittings, connnections and jointing material
	
	
	
	
	
	
	
	

	
	
	2
	x
	1
	300.00
	
	Total
	600.00
	Rft
	
	
	

	21
	Providing and fixing C.P brass shower having 1/2" (12 mm) dia inlet and 6" (150 mm) dia. detachable lid
	
	
	
	
	
	
	
	

	
	
	2
	x
	2
	
	
	
	4.00
	Each
	
	
	

	22
	Providing and fixing superior quality C.P. bib cock of approved make. 1/2" (12 mm) dia.
	
	
	
	
	
	
	
	

	
	
	2
	x
	6
	
	
	
	12.00
	Each
	
	
	

	23
	Providing and fixing Cement concrete gulley trap 6" x 6" x 4" (150 x 150 x 100 mm) with C.I. cover and frame weighing not less than 10 kg.
	
	
	
	
	
	
	
	

	
	
	2
	x
	6
	
	
	Total
	12.00
	No
	
	
	

	24
	Providing and fixing approved quality chromium plated towel rail with bracket and screws.
	
	
	
	
	
	
	
	

	
	
	2
	x
	4
	
	
	
	8.00
	No.
	
	
	

	25
	Providing and fixing approved quality C.P. brass toilet paper holder Master /Sonex or equivalent make.
	
	
	
	
	
	
	
	

	
	
	2
	x
	4
	
	
	
	8.00
	No.
	
	
	

	26
	Providing and fixing looking mirror of Belgium/ Malaysian/ Indonesian glass with chromium plated screws.
	
	
	
	
	
	
	
	

	
	
	2
	x
	2
	
	
	2.00
	8.00
	sft
	
	
	

	28
	Providing and fixing soap dish Chromium plated.
	
	
	
	
	
	
	
	

	
	
	2
	x
	2
	
	
	
	4.00
	No.
	
	
	

	29
	Providing and fixing 'P' trap including concrete chamber and C.I. grating Glazed 4" (100 mm) size.
	
	
	
	
	
	
	
	

	
	
	2
	x
	6
	
	
	
	12.00
	No
	
	
	

	
	Total Estimated Cost
	

	
	 BRA (Note)      
	

	
	Grand Total Amount (Inclusive of: All Taxes, Labour cost & Transportation charges) 
Note: BRA as per applicable percentage of 2nd schedule of Repair & Maintenance on payments other than Balochistan consolidated fund. 
	























































































	Dera Bugti Old Medicine Ware house Repair Renovation Work

	
	

	S.No
	DESCRIPTION
	Length (L)
	Width (W)
	Hieght (H)
	 QTY 
	UNIT
	 RATE 
	 AMOUNT 
	

	1
	Roofing 
	 
	 
	 
	 
	 
	 
	 
	

	 
	Providing and laying first class tile roof insulation comprising single layer of tiles12"x6"x1 1/2"grouted with cement sand mortar 1:3 laid over 2.5" thick cement concrete1:4:8 over glass wool /roof kool sheet wrapped in polythene sheet 300 gauge(0.03mm.)over a coat of PB-4 bitumen layer at the rate of 1.65 Kg./Sq.m.
	 
	 
	 
	 
	 
	 
	 
	

	 
	04 Rooms (16*14)
	17
	15
	 
	    1,020 
	 
	 
	 
	

	 
	01 Kitchen (16*14)
	17
	15
	 
	       255 
	 
	 
	 
	

	 
	01 Porch (10*10)
	10
	10
	 
	       100 
	 
	 
	 
	

	 
	Verandah (18*8)
	19
	9
	 
	       171 
	 
	 
	 
	

	 
	01 washrooms (8*5)
	9
	6
	 
	         54 
	 
	 
	 
	

	 
	 
	 
	 
	 
	    1,600 
	Sft
	 
	 
	

	2
	Girders & T iron
	 
	 
	 
	 
	 
	 
	 
	

	 
	Fabrication of heavy steel work with angle, tees, flat iron, round iron and sheet iron for making trusses, girders, tanks etc. including cutting, drilling riveting,handling,assembling and fixing but excluding erection in position as per directions of Engineer
	 
	 
	 
	 
	 
	 
	 
	

	 
	Girders (37Nos)
	14
	3
	 
	    1,554 
	 
	 
	 
	

	 
	T iron (90Nos)
	12
	0.5
	 
	       540 
	 
	 
	 
	

	 
	 
	 
	 
	 
	    2,094 
	kg 
	 
	 
	

	3
	Plaster 
	 
	 
	 
	 
	 
	 
	 
	

	 
	3/4 inch (19mm) thick cement plaster 1:3 using Coarse Sand on walls and columns in basement, plinth and ground floor including making edges, corners and curing.
	 
	 
	 
	 
	 
	 
	 
	

	 
	Building internal Plaster Patches need basis
	110
	 
	11
	    1,210 
	 
	 
	 
	

	 
	Building external Complete Plaster
	250
	 
	12
	    3,000 
	 
	 
	 
	

	 
	 
	 
	 
	 
	    4,210 
	Sft
	 
	 
	

	4
	Floor Concrete 
	 
	 
	 
	 
	 
	 
	 
	

	 
	Providing and laying plain machine mixed 1:3:6 cement concrete using coarse sand and crushed aggregate having maximum size upto 1-1/2" (38mm) & down gauge in foundation including levelling, compacting and curing.
	 
	 
	 
	 
	 
	 
	 
	

	 
	04 Rooms (16*14)
	16
	14
	0.50
	       448 
	 
	 
	 
	

	 
	01 Kitchen (16*14)
	16
	14
	0.50
	       112 
	 
	 
	 
	

	 
	Verandah (18*8)
	18
	8
	0.50
	         72 
	 
	 
	 
	

	 
	 
	 
	 
	 
	       632 
	Cft
	 
	 
	

	5
	Wiring
	 
	 
	 
	 
	 
	 
	 
	

	 
	Concealed/open wiring from point to switch with length upto 30 ft. (10m) including any switch to switch wiring with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables
	 
	 
	 
	 
	 
	 
	 
	

	 
	 
	 
	 
	 
	         30 
	Point
	 
	 
	

	6
	Distempering 
	 
	 
	 
	 
	 
	 
	 
	

	 
	Distempering with Berger, ICI or equivalent synthetic polyvinyl emulsion finish of
approved shade in two or more coats over and including the cost of priming coat including preparation of surface viz. dusting, sandpapering or rubbing with pumice
 stone, filling cracks or holes, ifany,removing blisters or other imperfections at any height and any floor. (@ at least 2.20 Liter per 10 Sq.m
	 
	 
	 
	 
	 
	 
	 
	

	 
	04 Rooms (16*14)
	16
	14
	11
	    3,536 
	 
	 
	 
	

	 
	01 Kitchen (16*14)
	16
	14
	11
	       884 
	 
	 
	 
	

	 
	Verandah (18*8)
	18
	8
	11
	       518 
	 
	 
	 
	

	 
	01 washrooms (8*5)
	8
	5
	11
	       326 
	 
	 
	 
	

	 
	 
	 
	 
	 
	    5,264 
	Sft
	 
	 
	

	7
	Weather Coat
	 
	 
	 
	 
	 
	 
	 
	

	 
	Applying weather resistant paint coating (Three coats (@ at least 3.00 Liter per 10 Sq.m)such as ICI/ Berger or equivalent paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning, scaffolding and removal of debris.
	 
	 
	 
	 
	 
	 
	 
	

	 
	Building external Complete Plaster
	250
	 
	12
	    3,000 
	 
	 
	 
	

	 
	 
	 
	 
	 
	    3,000 
	Sft
	 
	 
	

	 
	Total Estimated Amount
	 
	

	 
	BRA (Note)
	 
	

	 
	Total Amount
(Inclusive of: All Taxes, Labour cost & Transportation charges)
	 
	


Note: BRA as per applicable percentage of 2nd schedule of Repair & Maintenance on payments other than Balochistan consolidated.


























LOT 3
	
BHU Zahran Repair and Renovation

	S.No
	DESCRIPTION
	Length (L)
	Width (W)
	Hieght (H)
	QTY
	UNIT
	RATE
	
AMOUNT

	
	New Washroom (8*5)

	1
	Excavation
	
	
	
	
	
	
	

	
	Excavation in hard soil or soft murum in foundation of buildings and bridges including layout, dressing, refilling around structures with excavated earth, watering & ramming lead upto 100 ft. (30m) &
lift upto 5 ft. (1.5m)
	
	
	
	
	
	
	

	
	New Washroom (8*5)
	26
	2.50
	2
	130
	
	
	

	
	
	
	
	
	130
	Cu.ft
	
	

	2
	PCC (Lean Concrete)
	
	
	
	
	
	
	

	
	Providing and laying 1:4:8 plain machine mixed cement concrete using sand approved source and crushed aggregate having maximum size upto 1-1/2" (38mm) & down gauge in foundation and plinth including leveling, compacting & curing.
	
	
	
	
	
	
	

	
	New Washroom (8*5)
	26
	2.50
	0.250
	16.25
	
	
	

	
	
	
	
	
	16.25
	Cu.ft
	
	

	3
	Brick masonry
	
	
	
	
	
	
	

	
	Providing and laying first class solid burnt brick masonry cement sand 1 : 4 (Brick Strength: 1800psi-2000psi) including scaffolding, raking out joints and curing in ground floor superstructure and i/c cost of testing
	
	
	
	
	
	
	

	
	13.5" brick masonry
	26
	1.125
	2
	58.50
	
	
	

	
	
	
	
	
	58.50
	Cu.ft
	
	

	
	9" brick masonry
	26
	0.75
	10
	195
	
	
	

	
	
	
	
	
	195
	Cu.ft
	
	

	4
	Plaster
	
	
	
	
	
	
	

	
	3/4 inch (19mm) thick cement plaster 1:3 using Coarse Sand on walls and columns in basement, plinth and ground floor including making edges,
corners and curing.
	
	
	
	
	
	
	

	
	New Washroom (8*5) (inner/outer)
	26
	
	10
	520
	
	
	

	
	
	
	
	
	520
	Sft
	
	

	5
	Flooring
	
	
	
	
	
	
	

	
	Providing and laying plain machine mixed 1:3:6 cement concrete using coarse sand and crushed aggregate having maximum size upto 1-1/2" (38mm) & down gauge in foundation
	
	
	
	
	
	
	




	
	including levelling, compacting and curing.
	
	
	
	
	
	
	

	
	New Washroom (8*5)
	8
	5.00
	
	40
	Sft
	
	

	6
	Girders & T iron
	
	
	
	
	
	
	

	
	Fabrication of heavy steel work with angle, tees, flat iron, round iron and sheet iron for making trusses, girders, tanks etc. including cutting, drilling riveting,handling,assembling and fixing but excluding erection in position as per directions of
Engineer
	
	
	
	
	
	
	

	
	Girders (1Nos)
	14
	3
	
	42
	
	
	

	
	T iron (8Nos)
	12
	0.5
	
	48
	
	
	

	
	
	
	
	
	90
	kg
	
	

	7
	Roofing
	
	
	
	
	
	
	

	
	Providing and laying first class tile roof insulation comprising single layer of tiles12"x6"x1 1/2"grouted with cement sand mortar 1:3 laid over 2.5" thick cement concrete1:4:8 over glass wool /roof kool sheet wrapped in polythene sheet 300 gauge(0.03mm.)over a coat of PB-4
bitumen layer at the rate of 1.65 Kg./Sq.m.
	
	
	
	
	
	
	

	
	New Washroom (8*5)
	8
	5
	
	40
	
	
	

	
	
	
	
	
	40
	Sft
	
	

	8
	LDPE Water Tank
	
	
	
	
	
	
	

	
	Providing and fixing LDPE overhead tank 500 gallon capacity double ply, blue/white manufactured by Marjan, Master or equivalent on top of any
floor
	
	
	
	
	
	
	

	
	
	
	
	
	1
	Each
	
	

	9
	Distempering
	
	
	
	
	
	
	

	
	Distempering with Berger, ICI or equivalent synthetic polyvinyl emulsion finish ofapproved shade in two or more coats over and including the cost of priming coat including preparation of surface viz. dusting, sandpapering or rubbing with pumice stone, filling cracks or holes, ifany,removing blisters or other imperfections at any height and any floor. (@ at least 2.20 Liter per 10 Sq.m
	
	
	
	
	
	
	

	
	New Washroom (8*5)
	8
	5.00
	6
	196
	
	
	

	
	
	
	
	
	196
	Sft
	
	

	10
	Weather Coat
	
	
	
	
	
	
	

	
	Applying weather resistant paint coating (Three coats (@ at least 3.00 Liter per 10 Sq.m)such as ICI/ Berger or equivalent paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning,
scaffolding and removal of debris.
	
	
	
	
	
	
	



	
	Washrrom
	26
	
	11
	286
	
	
	

	
	
	
	
	
	286
	Sft
	
	

	11
	Tilling
	
	
	
	
	
	
	

	
	Providing and laying 1/4" to 3/8" (6mm to 9mm) thick Glazed/ Matt tiles of
any colour and size in ground floor laid over 1" (25mm) thick cement sand
mortar base including jointing and washing the tiles with white cement slurry of matching color by using
color pigment and curing.
	
	
	
	
	
	
	

	
	New Washroom (8*5)
	8
	5.00
	4
	144
	
	
	

	
	
	
	
	
	144
	Sft
	
	

	12
	Door Installation
	
	
	
	
	
	
	

	
	Providing and fixing fully glazed steel door with frame single leaf with M.S bottom or kick rail 6" (150mm) wide and top rail of 4" (100mm) wide painted  with  two  coats  of red oxide paint, brass oxidized fittings of lugs, cutting holed, andmaking good	the
damages to walls.
	
	
	
	
	
	
	

	
	
	
	
	
	21
	Sft
	
	

	13
	Windows Installation
	
	
	
	
	
	
	

	
	Providing and fixing hot dipped galvanized fully glazed double leaf hung steel windows and ventilators of approved section with Z-section
1.25" (32 mm) width at each
edge including using approved brass sections oxidized fitting, iron lugs, cutting holes and
making good the damages to walls.
	
	
	
	
	
	
	

	
	Windows type A
	2.5
	1.5
	
	3.75
	
	
	

	
	
	
	
	
	3.75
	Sft
	
	

	14
	Wiring
	
	
	
	
	
	
	

	
	Concealed/open wiring from point to switch with length upto 30 ft. (10m) including any switch to switch wiring with 3x1.5 Sq.mm PVC insulated single core copper conductor
Pakistan Cables, Pioneer, Newage or approved equivalent cables
	
	
	
	
	
	
	

	
	
	
	
	
	3
	Point
	
	

	15
	PPRC Pipes
	
	
	
	
	
	
	

	
	Providing, laying, cutting, jointing, testing and disinfecting PPRC pipes confirming to ISO 4427, PN- 20, complete in all respects
with specials and valves etc. including all fittings, connnections and jointing material
	
	
	
	
	
	
	

	
	
	
	
	
	30
	ft.
	
	

	16
	Wash Basins
	
	
	
	
	
	
	

	
	Providing and fixing approved quality fixtures Wash basin 24" (610 mm) ICL Futura make
	
	
	
	
	
	
	

	
	
	
	
	
	1
	No.
	
	




	17
	Water Closet
	
	
	
	
	
	
	

	
	Providing and fixing white English/indian W.C with glazed earthen ware 4"(100mm) trap squatting type water closet with integral treads ICL Boch/Karam Cera or approved equivalent make including cost of inlet pipe cistern and lid cistern kit, stop cock deluxe type and other accessories, fittings, brackets, PVC downpipe, rubber rings/washers, making requisite number of holes in walls, plinth and
floor for pipe connection and making good with approved material.
	
	
	
	
	
	
	

	
	
	
	
	
	1
	Each
	
	

	18
	UPVC sewerage pipes
	
	
	
	
	
	
	

	
	Providing and Installing uPVC pipe class b having 4"(100mm inner dia) IIL, Dadex or equivalent make registered with PSQCA in sewer lines and/or laying, cutting, jointing,
testing including all specials in pipe lines in trenches.
	
	
	
	
	
	
	

	
	
	
	
	
	20
	Rft
	
	

	19
	Soak Pit
	
	
	
	
	
	
	

	
	Providing and Construction of Soak Pit having diameter 3' with depth 10'
, inner filled with Brick ballast/stone ballast having RCC top , complete in all respects as per drawings and as
per direction of Engineer.
	
	
	
	
	
	
	

	
	
	
	
	
	1
	No
	
	

	20
	Washroom Assories set
	
	
	
	1
	each
	
	

	21
	Roof Screading
	
	
	
	
	
	
	

	
	Providing and laying 1:2:4 P.C.C roof screeding using crushed stone 3/4"
(19mm) including formwork, consolidation, finishing and curing
3" (75mm) nominal thick P.C.C. roof screeding
	
	
	
	
	
	
	

	
	BHU Building
	54
	15
	
	810
	
	
	

	
	
	
	
	
	810
	Sft
	
	

	22
	Plaster
	
	
	
	
	
	
	

	
	3/4 inch (19mm) thick cement plaster 1:3 using Coarse Sand on walls and columns in basement, plinth and ground floor including making edges, corners and curing.
	
	
	
	
	
	
	

	
	BHU interior (Patches need base)
	
	
	
	340
	
	
	

	
	BHU Building exterior
	
	
	
	1560
	
	
	

	
	
	
	
	
	1900
	Sft
	
	

	23
	Distempering
	
	
	
	
	
	
	




	
	Distempering with Berger, ICI or equivalent synthetic polyvinyl emulsion finish of
approved shade in two or more coats over and including the cost of priming coat including preparation of surface viz. dusting, sandpapering or rubbing with pumice
stone, filling cracks or holes, ifany,removing blisters or other imperfections at any height and any floor. (@ at least 2.20 Liter per 10
Sq.m
	
	
	
	
	
	
	

	
	Room-1
	14
	12
	11
	740
	
	
	

	
	Room-2
	14
	12
	11
	740
	
	
	

	
	Room-3
	14
	12
	11
	740
	
	
	

	
	
	
	
	
	2220
	Sft
	
	

	24
	Weather Coat
	
	
	
	
	
	
	

	
	Applying weather resistant paint coating (Three coats (@ at least 3.00 Liter per 10 Sq.m)such as ICI/ Berger or equivalent paint of approved shade on old surface of walls and ceiling including dusting,
sand papering and cleaning, scaffolding and removal of debris.
	
	
	
	
	
	
	

	
	BHU Building exterior
	130
	
	11
	1430
	
	
	

	
	
	
	
	
	1430
	Sft
	
	

	25
	Tilling
	
	
	
	
	
	
	

	
	Providing and laying 1/4" to 3/8" (6mm to 9mm) thick Glazed/ Matt tiles of
any colour and size in ground floor laid over 1" (25mm) thick cement sand
mortar base including jointing and washing the tiles with white cement slurry of matching color by using color pigment and curing.
	
	
	
	
	
	
	

	
	Room-1
	14
	12
	
	168
	
	
	

	
	Room-2
	14
	12
	
	168
	
	
	

	
	Room-3
	14
	12
	
	168
	
	
	

	
	
	
	
	
	504
	Sft
	
	

	
	Total Estimated Cost
	

	
	 BRA (Note)
	

	
	Total Amount
(Inclusive of: All Taxes, Labour cost & Transportation charges)
 Note: BRA as per applicable percentage of 2nd schedule of Repair & Maintenance on payments other than Balochistan consolidated fund.

	









LOT 4
	PPHI Balochistan

	DETAILED ESTIMATE FOR REHABILITATION AT DISTRICT PPHI UPPER DERA BUGTI

	

	S.
No.
	Description of work
	No.
	Measurement
	Quantity
	Unit
	Rate
	Amount

	
	
	
	Length
	Width
	Height
	
	
	
	

	5
	Providing and laying 1:2:4 P.C.C roof screeding using crushed stone 3/4" (19mm) including formwork, consolidation, finishing and curing. 1-1/2" (37.5mm) nominal thick P.C.C. roof screeding
	
	
	
	
	
	
	
	

	
	(SI No. 14-68 /c)
	
	
	
	
	
	
	
	
	
	
	

	
	Room 1
	1
	x
	1
	22.00
	13.00
	
	286.00
	Sft
	
	
	

	
	Room 2
	1
	x
	1
	18.00
	13.00
	
	234.00
	Sft
	
	
	

	
	Room 3
	1
	x
	1
	14.00
	12.00
	
	168.00
	Sft
	
	
	

	
	Room 4
	1
	x
	1
	13.50
	10.00
	
	135.00
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Total
	823.00
	Sft
	121.40
	P.Sft
	

	6
	Scraping, rubbing and cleaning of oil bound distemper from ceiling and walls including removal of rubbish in ground floor
	
	
	
	
	
	
	
	

	
	(SI No. 17-51-1)
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling
	
	
	
	
	
	
	
	
	
	
	

	
	Room 1
	1
	x
	1
	22.00
	13.00
	
	286.00
	Sft
	
	
	

	
	Room 2
	1
	x
	1
	18.00
	13.00
	
	234.00
	Sft
	
	
	

	
	Room 3
	1
	x
	1
	14.00
	12.00
	
	168.00
	Sft
	
	
	

	
	Room 4
	1
	x
	1
	13.50
	10.00
	
	135.00
	Sft
	
	
	

	
	Walls
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	2
	x
	1
	35.00
	
	12.00
	840.00
	Sft
	
	
	

	
	
	2
	x
	1
	31.00
	
	12.00
	744.00
	Sft
	
	
	

	
	
	2
	x
	1
	26.00
	
	12.00
	624.00
	Sft
	
	
	

	
	
	2
	x
	1
	23.50
	
	12.00
	564.00
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	TOTAL
	3595.00
	
	
	
	

	
	Projection
	1
	x
	1
	120.00
	2.50
	
	300.00
	Sft
	
	
	

	
	
	
	
	
	
	Sub Total
	3895.00
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	4
	x
	1
	3.50
	
	6.50
	91.00
	Sft
	
	
	

	
	D2
	2
	x
	1
	2.50
	
	6.50
	32.50
	Sft
	
	
	

	
	W1
	4
	x
	1
	4
	
	5.00
	80.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	203.50
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Net Qty.
	3691.50
	Sft
	8.74
	P.Sft
	

	7
	Distempering with Berger/ ICI or equivalent synthetic vinyl emulsion paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning in ground floor.
	
	
	
	
	
	
	
	

	
	(SI No. 17-60 b)
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling and Internal walls Quantity
	1
	x
	2
	3595.0
	
	Net Qty.
	7190.00
	Sft
	26.02
	P.Sft
	

	8
	Painting old surface in ground floor or basement with
	
	
	
	
	
	
	
	

	
	(SI No. 17-31 b)
	
	
	
	
	
	
	
	
	
	
	

	
	Qty of Door and Windows
	1
	x
	2
	
	
	Net Qty.
	203.50
	Sft
	35.77
	P.Sft
	

	9
	1/2 inch ( 13mm) thick cement plaster using Coarse Sand on wall sand columns in basement, plinth and ground floor including making edges, corners and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	S.I 15-3/ii
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	3895.0
	
	
	3895.00
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	4
	x
	1
	3.50
	
	6.50
	91.00
	Sft
	
	
	

	
	D2
	2
	x
	1
	2.50
	
	6.50
	32.50
	Sft
	
	
	

	
	W1
	4
	x
	1
	4.00
	
	5.00
	80.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	203.50
	Sft
	
	
	

	
	
	
	
	
	
	Net Total
	3691.50
	Sft
	62.45
	
	

	10
	Providing and laying 1:4:8 hand mixed cement concrete bed under floors using graded shingle or bajri 50 mm and down guage complete with levelling ramming watering and curing.
(S.I.No. 14-1/b)
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	22.00
	13.00
	0.25
	71.50
	cft
	
	
	

	
	
	1
	x
	1
	18.00
	13.00
	0.25
	58.50
	cft
	
	
	

	
	
	1
	x
	1
	14.00
	12.00
	0.25
	42.00
	cft
	
	
	

	
	
	1
	x
	1
	13.50
	10.00
	0.25
	33.75
	cft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	308.63
	cft
	332.92
	
	

	12
	Providing and laying 1/4" to 3/8" (6mm to 9mm) thick Glazed/ Matt tiles of any colour and size in ground floor laid over 1" (25mm) thick cement sand mortar base including jointing and washing the tiles with white cement slurry of matching color by using color pigment and curing
S.I No. 14-25 a
	
	
	
	
	
	
	
	

	
	Room
	1
	x
	1
	22.00
	13.00
	
	418.00
	cft
	
	
	

	
	Room
	1
	x
	1
	18.00
	13.00
	
	342.00
	cft
	
	
	

	
	Room
	1
	x
	1
	14.00
	12.00
	
	266.00
	cft
	
	
	

	
	Room
	1
	x
	1
	13.50
	10.00
	
	256.50
	cft
	
	
	

	
	
	
	
	
	
	
	
	1282.50
	sft
	278.29
	P.Sft
	

	
	Plumbing
	
	
	
	
	
	
	
	
	
	
	

	17
	Providing and fixing squatting type water closet with integral treads ICL Boch/Karam Cera or approved equivalent make including cost of inlet pipe cistern and lid cistern kit, stop cock deluxe type and other accessories, fittings, brackets, PVC down pipe, rubber rings/washers.
S.I No. 23-2 a-i
	
	
	
	
	
	
	
	

	
	
	
3
	
x
	
1
	
	
	
	
3.00
	
No
	
20653.99
	
P.No
	

	18
	Providing and fixing export quality glazed earthen ware wash basin manufactured by ICL Boch/Karam Cera or equivalent approved make with single hole chromium plated mixer tap 1/2" (15mm), pillar tap delux, stop cocks,
C.I. or W.I. brackets 6" (150mm) built into walls 1.5"
	
	
	
	
	
	
	
	

	
	S.I No. 23-5/ii
	3
	x
	1
	
	
	
	3.00
	No
	15440.40
	P.No
	

	19
	Providing, laying, cutting, jointing, testing and disinfecting PVC pipes confirming to BSS-3505/PS-3051 complete in all respects.
S.I No. 29-21 h
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	
	
	
	300.00
	Rft
	112.55
	P.RM
	

	20
	Providing, laying, cutting, jointing, testing and disinfecting PPRC pipes (25mm) confirming to ISO 4427, PN-20, complete in all respects with specials and valves etc. including all fittings, connnections and jointing material
S.I No. 27-46/a-iii
	
	
	
	
	
	
	
	

	
	
	3
	x
	1
	300.00
	
	Total
	900.00
	Rft
	715.35
	P.rft
	

	21
	Providing and fixing C.P brass shower having 1/2" (12 mm) dia inlet and 6" (150 mm) dia. detachable lid
	
	
	
	
	
	
	
	

	
	S.I No. 23-36 a
	3
	x
	2
	
	
	
	6.00
	Each
	4971.60
	Each
	

	22
	Providing and fixing superior quality C.P. bib cock of approved make. 1/2" (12 mm) dia.
S.I No. 23-34 a
	
	
	
	
	
	
	
	

	
	
	3
	x
	6
	
	
	
	18.00
	Each
	1018.80
	Each
	

	23
	Providing and fixing Cement concrete gulley trap 6" x 6" x 4" (150 x 150 x 100 mm) with C.I. cover and frame weighing not less than 10 kg.
S.I No. 25-2 a
	
	
	
	
	
	
	
	

	
	
	3
	x
	6
	
	
	Total
	18.00
	No
	6952.05
	each
	

	24
	Providing and fixing approved quality chromium plated towel rail with bracket and screws.
	
	
	
	
	
	
	
	

	
	S.I No. 23-13 a
	3
	x
	4
	
	
	
	12.00
	No.
	115.83
	each
	

	25
	Providing and fixing approved quality C.P. brass toilet paper holder Master /Sonex or equivalent make.
	
	
	
	
	
	
	
	

	
	S.I No. 23-14
	3
	x
	4
	
	
	
	12.00
	No.
	1632.00
	each
	

	26
	Providing and fixing looking mirror of Belgium/ Malaysian/ Indonesian glass with chromium plated screws.
	
	
	
	
	
	
	
	

	
	S.I No. 23-15
	3
	x
	2
	
	
	2.00
	12.00
	sft
	2569.20
	P.sft
	

	28
	Providing and fixing soap dish Chromium plated.
	
	
	
	
	
	
	
	

	
	S.I No. 23-29 a
	3
	x
	2
	
	
	
	6.00
	No.
	531.60
	each
	

	29
	Providing and fixing 'P' trap including concrete chamber and C.I. grating Glazed 4" (100 mm) size.
	
	
	
	
	
	
	
	

	
	S.I No. 23-42 b
	3
	x
	6
	
	
	
	18.00
	No
	2312.40
	P.No
	

	
	
	
	

	
	TOTAL(Rs.)
	
	

	
	Say in Million Rs.
	
	












































	PPHI Balochistan

	DETAILED ESTIMATE FOR REHABILITATION AT DISTRICT PPHI UPPER DERA BUGTI

	CONSTRUCTION OF BOUNDARY WALL

	S.
No.
	Description of work
	No.
	Measurement
	Quantity
	Unit
	Rate
	Amount

	
	
	
	Length
	Width
	height
	
	
	
	

	7
	Providing and laying 1:4:8 cement concrete block masonry using coarse sand and approved crushed aggregate 3/4" (19 mm) and down gauge in ground floor superstructure, including scaffolding, raking out joints, and curing.
S.I No. 11-12 b-iii
	
	
	
	
	
	
	
	

	
	Wall
	1
	x
	1
	170.00
	0.5
	2.00
	170.00
	cft
	
	
	

	
	
	
	
	
	
	
	Net
	170.00
	cft
	442.65
	P.cft
	

	8
	Providing and laying 1:2:4 cement concrete using approved coarse sand and crushed aggregate 3/4" (19mm) and down gauge in coping, including formwork & its removal, compacting and curing in ground floor.
S.I No. 5-27 a
	
	
	
	
	
	
	
	

	
	Coping
	1
	x
	1
	170.00
	0.5
	0.25
	21.25
	cft
	518.27
	P.cft
	

	9
	3/4 inch (19mm) thick cement plaster 1:4 using Coarse Sand on walls and columns in ground floor including making edges, corners and curing.
S.I No. 15-4 iii
	
	
	
	
	
	
	
	

	
	Walls
	2
	x
	4
	170.00
	
	2.00
	2720.00
	sft
	
	
	

	
	
	
	
	
	
	
	Total
	2720.00
	sft
	62.56
	P.Sft
	

	10
	Providing and fixing collapsible steel shutter or gate with vertical channels, flat iron diagonal, top and bottom rail with steel rollers of required size, T-iron bottom track riveting the junctions, including locking arrangement and handles, cutting holes, painting two coats of red oxide paint, fixing bottom track with cement concrete 1:2:4 and making good the damages to walls fabrication as designed and erectionas per instructions of the Engineer Incharge.
S.I No. 28-85 a
	
	
	
	
	
	
	
	

	
	Gate
	1
	x
	1
	10.00
	
	4.00
	40.00
	sft
	
	
	

	
	
	
	
	
	
	
	Total
	40.00
	sft
	725.71
	P.sft
	

	11
	Applying weather resistant paint coating such as ICI weather shield,Berger weather coat or equivalent to interior or exterior walls or ceiling including supplying all labour, materials, scaffoldings and removal of debris etc. @ atleast 3.50 litre per 10
S.I No. 17-69
	
	
	
	
	
	
	
	

	
	Walls
	1
	x
	4
	170.00
	
	2.00
	1360.00
	sft
	
	
	

	
	
	
	
	
	
	
	Total
	1360.00
	sft
	80.77
	P.Sft
	

	12
	Painting with ICI/Berger or equivalent super gloss synthetic enamel paint in two or more coats as per manufacturer's instructions on steel and iron work over and including the cost of priming coat, surface preparation, removing rust, scales and dust with wire brush in ground floor or basement. (@ atleast 1.25Litre per 10 Sq.m)
S.I No. 17-7
	
	
	
	
	
	
	
	

	
	Gate
	1
	x
	2
	10.00
	
	4.00
	20.00
	sft
	
	
	

	
	
	
	
	
	
	
	Total
	20.00
	sft
	59.85
	P.Sft
	

	
	Total
	














	PPHI Balochistan

	DETAILED ESTIMATE FOR REHABILITATION AT DISTRICT PPHI UPPER DERA BUGTI

	

	S.
No.
	Description of work
	No.
	Measurement
	Quantity
	Unit
	Rate
	Amount

	
	
	
	Length
	Width
	Height
	
	
	
	

	

2
	
Providing rolled steel joists and channels including hoisting and fixing in position in cement concrete but excluding the cost of cement concrete
	
	
	
	
	
	
	
	
	
	
	

	
	SI No 28-32
	
	
	
	
	
	
	
	
	
	
	

	
	Bath
	3
	x
	1
	6.00
	6
	
	108.00
	kgs
	
	
	

	
	
	
	
	
	
	
	
	108.00
	
	394.18
	
	

	3
	Providing M.S. Tees, angles and flats including fixing
in position.
	
	
	
	
	
	
	
	
	
	
	

	
	SI No 28-33
	
	
	
	
	
	
	
	
	
	
	

	
	Bath
	3
	x
	1
	6.00
	6.00
	1.50
	162.00
	lbs
	
	
	

	
	
	
	
	
	
	
	
	162.00
	lbs
	
	
	

	
	
	
	
	5406/2.204
	
	
	73.50
	kg
	406.97
	
	

	




4
	Providing and laying second class brick tile roofing comprising 4 inches (100mm) thick earth and 1 inch (25 mm) thick mud plaster with gobri leeping over 1/2 inch (13mm) thick cement plaster 1:6 with 34 lbs./100 Sq.ft.(1.65 Kg./Sq.m.) hot bitumen coating sand blended in one coat, provided over one layer of tiles 12" x 6"x 2" laid in 1:6 cement sand mortar including 1:2 cement sand pointing underside of tiles including curing
	
	
	
	
	
	
	
	
	
	
	

	
	SI No 13-2/b
	
	
	
	
	
	
	
	
	
	
	

	
	Bath
	3
	x
	1
	7.50
	7.50
	
	168.75
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	168.75
	Sft
	204.82
	
	

	5
	Providing and laying 1:2:4 P.C.C roof screeding using crushed stone 3/4" (19mm) including formwork, consolidation, finishing and curing. 1-1/2" (37.5mm) nominal thick P.C.C. roof screeding
	
	
	
	
	
	
	
	

	
	(SI No. 14-68 /c)
	
	
	
	
	
	
	
	
	
	
	

	
	Bath
	2
	x
	1
	7.50
	7.50
	
	112.50
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	112.50
	Sft
	121.40
	P.Sft
	

	6
	Scraping, rubbing and cleaning of oil bound distemper from ceiling and walls including removal of rubbish in ground floor
	
	
	
	
	
	
	
	

	
	(SI No. 17-51-1)
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling
	
	
	
	
	
	
	
	
	
	
	

	
	Bath
	3
	x
	1
	7.50
	7.50
	
	168.75
	Sft
	
	
	

	
	Walls
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	3
	x
	4
	15.00
	
	12.00
	2160.00
	Sft
	
	
	

	
	
	
	
	
	
	
	TOTAL
	2328.75
	
	
	
	

	
	Projection
	1
	x
	1
	120.00
	2.50
	
	300.00
	Sft
	
	
	

	
	
	
	
	
	
	Sub Total
	2628.75
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	3
	x
	1
	3.50
	
	6.50
	68.25
	Sft
	
	
	

	
	D2
	3
	x
	1
	2.50
	
	6.50
	48.75
	Sft
	
	
	

	
	V
	3
	x
	1
	2
	
	2.00
	12.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	129.00
	Sft
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Net Qty.
	2499.75
	Sft
	8.74
	P.Sft
	

	7
	Distempering with Berger/ ICI or equivalent synthetic vinyl emulsion paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning in ground floor.
	
	
	
	
	
	
	
	

	
	(SI No. 17-60 b)
	
	
	
	
	
	
	
	
	
	
	

	
	Ceiling and Internal walls Quantity
	1
	x
	2
	2328.8
	
	Net Qty.
	4657.50
	Sft
	26.02
	P.Sft
	

	8
	Painting old surface in ground floor or basement with
	
	
	
	
	
	
	
	

	
	(SI No. 17-31 b)
	
	
	
	
	
	
	
	
	
	
	

	
	Qty of Door and Windows
	1
	x
	2
	
	
	Net Qty.
	129.00
	Sft
	35.77
	P.Sft
	

	9
	1/2 inch ( 13mm) thick cement plaster using Coarse Sand on wall sand columns in basement, plinth and ground floor including making edges, corners and curing.
	
	
	
	
	
	
	
	
	
	
	

	
	S.I 15-3/ii
	
	
	
	
	
	
	
	
	
	
	

	
	
	1
	x
	1
	2628.8
	
	
	2628.75
	Sft
	
	
	

	
	Deduction
	
	
	
	
	
	
	
	
	
	
	

	
	D
	3
	x
	1
	3.50
	
	6.50
	68.25
	Sft
	
	
	

	
	D2
	3
	x
	1
	2.50
	
	6.50
	48.75
	Sft
	
	
	

	
	V
	3
	x
	1
	2.00
	
	2.00
	12.00
	Sft
	
	
	

	
	
	
	
	
	
	
	Total
	129.00
	Sft
	
	
	

	
	
	
	
	
	
	Net Total
	2499.75
	Sft
	62.45
	
	

	10
	Providing and laying 1:4:8 hand mixed cement concrete bed under floors using graded shingle or bajri 50 mm and down guage complete with levelling ramming watering and curing.
(S.I.No. 14-1/b)
	
	
	
	
	
	
	
	
	
	
	

	
	
	3
	x
	1
	6.00
	6.00
	0.25
	27.00
	cft
	
	
	

	
	
	
	
	
	
	
	
	40.50
	cft
	332.92
	
	

	11
	Providing and fixing 1/4" to 3/8" (6mm to 9mm) thick Ceramic Glazed/Matt tiles (Prime Quality) of any colour and  size,  as  directed  by  Engineer-in-Charge  in dado/skirting in ground floor over 1/2" (13mm) thick base of cement mortar 1:3, setting of tiles in slurry of grey cement over mortar base including filling the joints and washing the tiles with white cement slurry of matching color, cleaning & curing.
S.I No. 14-64 a
	
	
	
	
	
	
	
	

	
	Bath
	3
	x
	4
	6.00
	
	7.00
	504.00
	sft
	
	
	

	
	Deduction
	
	
	
	
	
	Total
	655.20
	sft
	
	
	

	
	d1
	3
	x
	1
	2.50
	
	6.50
	48.75
	sft
	
	
	

	
	
	
	
	
	
	
	Total
	48.75
	sft
	
	
	

	
	
	
	
	
	
	
	Net Qty
	606.45
	sft
	213.60
	P.Sft
	

	12
	Providing and laying 1/4" to 3/8" (6mm to 9mm) thick Glazed/ Matt tiles of any colour and size in ground floor laid over 1" (25mm) thick cement sand mortar base including jointing and washing the tiles with white cement slurry of matching color by using color pigment and curing
S.I No. 14-25 a
	
	
	
	
	
	
	
	

	
	Bath
	2
	x
	1
	6.00
	6.00
	
	228.00
	cft
	
	
	

	
	
	
	
	
	
	
	
	228.00
	sft
	278.29
	P.Sft
	

	
	ELECTRICAL WORK
	
	
	
	
	
	
	
	
	
	
	

	15
	Concealed wiring from point to switch with 3/4" (20 mm)  dia.  PVC  conduit length upto 30 ft. (10m) including any switch to switch wiring with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables,
	
	
	
	
	
	
	
	

	
	S.I No. 30-3 a
	3
	x
	1
	
	
	
	3.00
	Point
	4278.60
	P.Poin
	

	16
	Concealed wiring for 5 Amp. Socket outlets from nearest available circuit with 3/4" (20 mm) dia. PVC conduit length upto 20 ft. (6m) with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables
	
	
	
	
	
	
	
	

	
	S.I No. 30-8 a
	3
	x
	1
	
	
	
	3.00
	Point
	3358.32
	P.Poin
	

	17
	Supply and install 2-gang, 5 Amp, 250 Volt,. plate type moulded switch including appropriate size plastic box to be fixed recessed in wall.
	
	
	
	
	
	
	
	

	
	S.I No. 30-12
	1
	x
	1
	
	
	
	1.00
	No.
	897.80
	each
	

	18
	Supply and install combined 2/3 pin 5 Amps, 250 Volt switch socket unit including plastic box to be fixed recessed in wall.
	
	
	
	
	
	
	
	

	
	S.I No. 30-19
	3
	x
	1
	
	
	
	3.00
	No.
	1732.44
	each
	

	19
	Supply and install Energy Saver electric bulbs
	
	
	
	
	
	
	
	
	
	
	

	
	S.I No. 30-117 c
	3
	x
	1
	
	
	
	3.00
	No.
	436.00
	P.No
	

	20
	Supply and install 10" (250 mm) sweep exhaust fan
including plastic louvers.
	
	
	
	
	
	
	
	

	
	S.I No. 30-113
	3
	x
	1
	
	
	
	3.00
	No.
	5564.40
	each
	

	21
	Installing each number circuit breaker 6 Ampere on same distribution board and bus bar (For outgoing)
	
	
	
	
	
	
	
	

	
	S.I No. 30-116 b
	3
	x
	2
	
	
	
	6.00
	No.
	3621.00
	P.job
	

	
	
	
	
	
	TOTAL(Rs.)
(Inclusive of: All Taxes, Labour cost & Transportation charges)
	
	

	
	
	
	BRA.
	
	


Note: BRA as per applicable percentage of 2nd schedule of Repair & Maintenance on payments other than Balochistan consolidated fund.






















LOT 5
	District Office Barshore Repair and Renovation Work

	S.No
	DESCRIPTION
	Length
(L)
	Width
(W)
	Hieght
(H)
	QTY
	UNIT
	RATE
	AMOUNT

	1
	Ground Clearance and leveling
	
	
	
	
	
	
	

	
	Levelling and dressing the ground by cutting and filling of earth in depth upto 6
inches including consolidating. (Rough
Levelling in Ordinary Soil) Sloppy Area.
	
	
	
	
	
	
	

	
	
	
	
	
	500
	Sq.ft
	15.00
	

	2
	Excavation
	
	
	
	
	
	
	

	
	Excavation in foundation of buildings and bridges including layout, dressing, refilling around structures with excavated earth, watering & ramming lead upto 100 ft. (30m)
& lift upto 5 ft. (1.5m)
	
	
	
	
	
	
	

	
	Additional Room (16*14)
	60
	2.50
	2
	300
	
	
	

	
	New Washroom (8*6) 01 Nos
	28
	2.50
	2
	140
	
	
	

	
	
	
	
	
	440
	Cu.ft
	16.09
	

	3
	PCC (Lean Concrete)
	
	
	
	
	
	
	

	
	Providing and laying plain hand mixed cement concrete using sand approved source and crushed aggregate having maximum size upto 1-1/2" (38mm) & down gauge in foundation and plinth including
leveling, compacting & curing.
	
	
	
	
	
	
	

	
	New Washroom (8*6) 01 Nos
	28
	2.50
	0.250
	17.50
	
	
	

	
	Additional Room (16*14)
	60
	2.50
	0.250
	37.50
	
	
	

	
	
	
	
	
	55.00
	Cu.ft
	400.56
	

	4
	Reinforced cement concrete
	
	
	
	
	
	
	

	
	8 nos columns for Room and washroom 9" *
9" main bar # 4 stirups  # 3 @ 6 c/c
	0.75
	0.75
	12.00
	300.09
	kg
	275.00
	

	
	Door band for room and washrooms 9" * 9"
main bar # 4 stirups  # 3 @ 6 c/c
	88.00
	0.75
	0.75
	220.06
	kg
	275.00
	

	
	concreting
	
	
	
	
	
	
	

	
	Room+washroom Columns
	0.75
	0.75
	12.00
	54.00
	
	
	

	
	Door band
	88.00
	0.75
	0.75
	49.50
	
	
	

	
	
	
	
	
	103.50
	Cu.ft
	330.00
	

	5
	Brick masonry
	
	
	
	
	
	
	

	
	Providing and laying first class solid burnt brick masonry (Brick Strength:1400psi-1700psi) including scaffolding, raking out joints and curing in foundation and substructure/Basement i/c cost of testing Above 4.5" thick brickwork upto any thickness
Cement sand 1 : 4
	
	
	
	
	
	
	

	
	New Washroom (8*6) 01 Nos
	28
	1.125
	2
	63.00
	
	
	

	
	
	28
	0.75
	10
	210.00
	
	
	

	
	Additional Room (16*14)
	60
	1.125
	2
	135.00
	
	
	

	
	
	60
	0.75
	10
	450.00
	
	
	

	
	
	
	
	
	858.00
	Cu.ft
	457.95
	

	6
	Plaster
	
	
	
	
	
	
	

	
	3/4 inch (19mm) thick cement plaster 1:3 using Coarse Sand on walls and columns in basement, plinth and ground floor including making edges, corners and curing.
	
	
	
	
	
	
	

	
	New Washroom (8*6) 01 Nos
	28
	
	10
	560
	
	
	

	
	Additional Room (16*14)
	60
	
	10
	1200
	
	
	

	
	
	
	
	
	1760
	Sft
	65.73
	

	7
	Flooring
	
	
	
	
	
	
	

	
	Providing and laying 1:2:4 cement concrete floor using using crushed
aggrgate 3/4" (19mm) and down gauge in ground floor laid in panels
including formwork, consolidation, finishing and curing.
4" (100 mm) nominal thick flooring
	
	
	
	
	
	
	

	
	New Washroom (8*6) 01 Nos
	8
	6.00
	
	48
	
	
	

	
	Additional Room (16*14)
	16
	14.00
	
	224
	
	
	

	
	
	
	
	
	272
	Sft
	188.66
	

	8
	Girders & T iron
	
	
	
	
	
	
	

	
	Fabrication of heavy steel work with angle, tees, flat iron, round iron and sheet iron for making trusses, girders, tanks etc. including cutting, drilling riveting,handling,assembling and fixing but excluding erection in position as per directions of Engineer
	
	
	
	
	
	
	

	
	Girders (7Nos)
	14
	3
	
	294
	
	
	

	
	T iron (24Nos)
	12
	0.5
	
	144
	
	
	

	
	
	
	
	
	438
	kg
	380.63
	

	9
	Roofing
	
	
	
	
	
	
	

	
	Providing and laying first class tile roof insulation comprising single layer of tiles12"x6"x1 1/2"grouted with cement sand mortar 1:3 laid over 2.5" thick cement concrete1:4:8 over glass wool /roof kool sheet wrapped in polythene sheet 300 gauge(0.03mm.)over a coat of PB-4 bitumen layer at the rate of 1.65 Kg./Sq.m.
	
	
	
	
	
	
	

	
	New Washroom (8*6) 01 Nos
	8
	6.00
	
	48
	
	
	

	
	Additional Room (16*14)
	16
	14.00
	
	224
	
	
	

	
	
	
	
	
	272
	Sft
	267.26
	

	10
	Roof Screading
	
	
	
	
	
	
	

	
	Providing and laying 1:2:4 P.C.C roof screeding using crushed stone 3/4" (19mm) including formwork, consolidation, finishing and curing
3" (75mm) nominal thick P.C.C. roof
screeding
	
	
	
	
	
	
	

	
	New Washroom (8*6) 01 Nos
	8
	6.00
	
	48
	
	
	

	
	Additional Room (16*14)
	16
	14.00
	
	224
	
	
	

	
	BHU Building
	36
	34.00
	
	1224
	
	
	

	
	
	
	
	
	1496
	Sft
	137.94
	

	11
	LDPE Water Tank
	
	
	
	
	
	
	

	
	Providing and fixing LDPE overhead tank 500 gallon capacity double ply, blue/white manufactured by Marjan, Master or
equivalent on top of any floor
	
	
	
	
	
	
	

	
	
	
	
	
	1
	Each
	32,428.80
	

	12
	Distempering
	
	
	
	
	
	
	

	
	Distempering with Berger, ICI or equivalent synthetic polyvinyl emulsion finish of approved shade in two or more coats over and including the cost of priming coat including preparation of surface viz. dusting, sandpapering or rubbing with pumice
stone, filling cracks or holes, ifany,removing blisters or other imperfections at any height and any floor. (@ at least 2.20 Liter per 10 Sq.m
	
	
	
	
	
	
	

	
	New Washroom (8*6) 01 Nos
	8
	6.00
	5
	188
	
	
	

	
	Existing Washroom (8*6) 01 Nos
	8
	6.00
	5
	188
	
	
	

	
	Additional Room (16*14)
	16
	14.00
	10
	824
	
	
	

	
	Room-1
	18
	14.00
	10
	892
	
	
	

	
	Room-2
	14
	12.00
	10
	688
	
	
	

	
	Room-3
	14
	12.00
	10
	688
	
	
	

	
	Store
	8
	8.00
	10
	384
	
	
	

	
	Kitchen
	12
	10.00
	10
	560
	
	
	

	
	Verandah
	14
	8.00
	10
	472
	
	
	

	
	
	
	
	
	4884
	Sft
	44.69
	

	13
	Roof Ceilng
	
	
	
	
	
	
	

	
	Providing and fixing Gypsum Board false ceiling of approved size and
texture consisting of imported powder coated aluminum angle and
tee framing (size 1" x 1") hunged by approved suspension system,
including provision of extra framing for lights fittings, A/C diffusers
and around columns, etc, complete in all respectas directed by the
Engineer. (1/4" (6.4 mm) thick laminated
gypsum board)
	
	
	
	
	
	
	

	
	Additional Room (16*14)
	16
	14.00
	
	224
	
	
	

	
	
	
	
	
	224
	Sq.ft
	134.15
	

	14
	Weather Coat
	
	
	
	
	
	
	

	
	Applying weather resistant paint coating (Three coats (@ at least 3.00 Liter per 10 Sq.m)such as ICI/ Berger or equivalent paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning, scaffolding and removal of
debris.
	
	
	
	
	
	
	

	
	New Washroom (8*6) 01 Nos
	28
	
	11
	308
	
	
	

	
	BHU Building+Additional Room
	170
	
	12
	2040
	
	
	

	
	
	
	
	
	2348
	Sft
	67.39
	

	15
	Tilling
	
	
	
	
	
	
	

	
	Providing and laying 1/4" to 3/8" (6mm to 9mm) thick Glazed/ Matt tiles of
any colour and size in ground floor laid over 1" (25mm) thick cement sand
mortar base including jointing and washing the tiles with white cement
slurry of matching color by using color
pigment and curing.
	
	
	
	
	
	
	

	
	Washroom (8*6) 01 Nos new + 01 existing
	8
	6.00
	4
	320
	
	
	

	
	Room-1
	18
	14.00
	0.5
	284
	
	
	

	
	Room-2
	14
	12.00
	0.5
	194
	
	
	

	
	Room-3
	14
	12.00
	0.5
	194
	
	
	

	
	Verandah
	14
	8.00
	0.5
	130
	
	
	

	
	
	
	
	
	1122
	Sft
	381.08
	

	16
	Door Frame Installation
	
	
	
	
	
	
	

	
	Providing and fixing moulded steel door frame of approved profile, manufactured from
zinc-coated mild steel sheets 16 gauge made by Shahah Industries or equivalent standard
conforming to B.S.S.1245, treated with special primer base paint all round, fitted with six
fixing lugs, three steel hinges for fixing door shutters standard lock-strike plate, one sliding
holt eye, and three rubber buffers, including cutting holes and making good damages to walls and filling the door frame cavity with lean cement mortar 1:4 as directed by the Engineer Incharge.
	
	
	
	
	
	
	

	
	Washroom 01 Nos
	7
	3
	
	17
	
	
	

	
	Room 01 Nos
	7
	3.5
	
	17.5
	
	
	

	
	
	
	
	
	34.50
	Rft
	663
	

	17
	Door Installation
	
	
	
	
	
	
	

	
	Providing and fixing 1.5" (38mm) thick pressed Teak wood, 5 Ply flushed with First class wood veneering on all faces and sides fixed over deodar wood cavited core and frame work of not less than 4" (100mm) wide strips all-round with approved brass hinges, tower bolts as required
	
	
	
	
	
	
	

	
	Washroom 01 Nos
	7
	3
	
	21
	
	
	

	
	Room 01 Nos
	7
	3.5
	
	24.5
	
	
	

	
	
	
	
	
	45.5
	Sft
	1,360.45
	

	18
	Windows Installation
	
	
	
	
	
	
	

	
	Providing and fixing hot dipped galvanized fully glazed double leaf hung steel windows and ventilators of approved section with Z-section 1.25" (32 mm) width at each
edge including using approved brass sections oxidized fitting, iron lugs, cutting holes and
making good the damages to walls.
	
	
	
	
	
	
	

	
	ventilators 01 Nos
	2.5
	1.5
	
	3.75
	
	
	

	
	Windows 01 Nos
	6
	4
	
	24
	
	
	

	
	
	
	
	
	27.75
	Sft
	1,397.13
	

	19
	Wiring
	
	
	
	
	
	
	

	
	Concealed/open wiring from point to switch with length upto 30 ft. (10m) including any switch to switch wiring with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables
	
	
	
	
	
	
	

	
	
	
	
	
	15
	Point
	4,278.60
	

	20
	PPRC Pipes
	
	
	
	
	
	
	

	
	Providing, laying, cutting, jointing, testing and disinfecting PPRC
pipes confirming to ISO 4427, PN-20, complete in all respects
with specials and valves etc. including all fittings, connnections
and jointing material
	
	
	
	
	
	
	

	
	
	
	
	
	80
	ft.
	428.56
	

	21
	Wash Basins
	
	
	
	
	
	
	

	
	Providing and fixing approved quality fixtures Wash basin 24" (610 mm) ICL Futura make
	
	
	
	
	
	
	

	
	
	
	
	
	2
	No.
	10,000.00
	

	22
	Water Closet
	
	
	
	
	
	
	

	
	Providing and fixing white English W.C with glazed earthen ware 4"(100mm) trap squatting type water closet with integral treads ICL Boch/Karam Cera or approved equivalent make including cost of inlet pipe cistern and lid cistern kit, stop cock deluxe type and other accessories, fittings, brackets, PVC downpipe, rubber rings/washers, making requisite number of holes in walls, plinth and floor for pipe connection and making good with approved
material.
	
	
	
	
	
	
	

	
	
	
	
	
	2
	Each
	20,500.00
	

	23
	UPVC sewerage pipes
	
	
	
	
	
	
	

	
	Providing and Installing uPVC pipe class b having 4"(100mm inner dia) IIL, Dadex or equivalent make registered with PSQCA in sewer lines and/or laying, cutting, jointing, testing including all specials in pipe lines in
trenches.
	
	
	
	
	
	
	

	
	
	
	
	
	60
	Rft
	804.31
	

	24
	Soak Pit
	
	
	
	
	
	
	

	
	Providing and Construction of Soak Pit having diameter 3' with depth 10' , inner filled with Brick ballast/stone ballast having RCC top , complete in all respects as per drawings and as per direction of Engineer.
	
	
	
	
	
	
	

	
	
	
	
	
	1
	No
	45,000.00
	

	25
	Washroom Assories set
	
	
	
	2
	each
	12,000.00
	

	26
	Complete Solar System (2.5 KW)
	
	
	
	
	
	
	

	
	Inverex inverter 2.5 KW
	
	
	
	1
	
	145,000.00
	

	
	Solar Panel (Longi A Grade 585/W)
	
	
	
	5
	
	31,000.00
	

	
	Solar Stand Frame (14 gauge)
	
	
	
	2
	
	30,000.00
	

	
	Cable 6mm
	
	
	
	1
	
	25,000.00
	

	
	Phoenex Tubular Batteries TR 1800 (185
AH)
	
	
	
	2
	
	75,000.00
	

	
	Breaker Board, DB Box and other accessories One set complete in all respect
	
	
	
	
1
	
	
25,000.00
	

	
	
	
	
	
	
	
	
	

	27
	Tuff Tilling
	
	
	
	
	
	
	

	
	Supply and Fixing of Concrete pavers on sand cushion of different designs
having thickness of 50 mm, mechnically compressed, minimium strenght of
4500 psi after laboratory testing at factory and random testiing at site as
and when desired by the Engineer inchange
comple in all respects. (50mm thick,tuff tile Cloured)
	
	
	
	
	
	
	

	
	
	36
	20.00
	
	720
	Sft
	179.34
	

	28
	Main Gate Installation
	
	
	
	
	
	
	

	
	Providing and fixing steel grated double leaf Gate with locking arrangement, and angle iron (2" x 2" x .375") for frame, middle strip 6.4 mm (.25) thick gusset plate 75 mm
x 75 mm (3" x 3" ) at each edge and 19 mm (.75) M.S square or round bars 5/8" or 6/8" dia at 100 mm (4) center to center including two coats of red oxide paint as per the direction of Engineer Incharge.
	
	
	
	
	
	
	

	
	
	12
	8.00
	
	96
	sqft
	2367.94
	

	29
	Sign Board and Direction Board
	
	
	
	
	
	
	

	
	Installation and fixation of Sign Board 10x2 ,
Dirction Board 4x4.
	
	
	
	1
	job
	60,000.00
	

	30
	Underground Water Tank (UGWT)
	
	
	
	
	
	
	

	
	Circular underground water tank Dia 6' and
10' deep, complete in all respect.
	
	
	
	1
	job
	100,000.00
	

	
	Total Estimated Cost
	

	
	BRA
	

	
	Note: BRA as per applicable percentage of 2nd schedule of Repair & Maintenance on payments other than Balochistan consolidated fund.


	

















Page 109 of 110

image2.jpeg
PPHI




image3.jpeg
PPHI




image1.jpg
PPHI-B




